| dfeprach Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfePrach_CarrierCfg Struct Reference
Overview

Configuration for a single CC. More...

## Data Fields
u32 | SCS
      [0-4] Array of SCS values, one  for each CCID number
(different index from the location that the sequence is mapped to). More...

## Detailed Description

Configuration for a single CC.

## Field Documentation

u32 XDfePrach_CarrierCfg::SCS

      [0-4] Array of SCS values, one  for each CCID number

(different index from the location that the sequence is mapped to).

Sub carrier Spacing for each CC - required to determine Slot boundaries:

- 0: 15KHz spacing
- 1: 30KHz spacing
- 2: 60KHz spacing
- 3: 120KHz spacing
- 4: 240KHz spacing

Referenced by XDfePrach_2CC3RCDynamicTestExample(), XDfePrach_2CC3RCReconfigureTestExample(), XDfePrach_2CC3RCTestExample(), XDfePrach_AddCCtoCCCfgMB(), XDfePrach_GetCarrierCfgMB(), XDfePrach_GetCCMB(), and XDfePrach_UpdateCCinCCCfgMB().