| hwicap Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XHwIcap_Config Struct Reference
Overview

This typedef contains configuration information for the device. More...

## Data Fields
u16 | DeviceId
| Device ID of device. More...
UINTPTR | BaseAddress
| Register base address. More...
int | IcapWidth
| Width of ICAP. More...
int | IsLiteMode
| IsLiteMode, 0 not present, 1 present. More...

## Detailed Description

This typedef contains configuration information for the device.

## Field Documentation

UINTPTR XHwIcap_Config::BaseAddress

Register base address.

Referenced by HwIcapIntrExample(), HwIcapReadConfigRegExample(), HwIcapReadFramePolledExample(), HwIcapTestAppExample(), XHwIcap_Abort(), XHwIcap_CfgInitialize(), XHwIcap_DeviceRead(), XHwIcap_DeviceWrite(), XHwIcap_FlushFifo(), XHwIcap_GetConfigReg(), XHwIcap_Reset(), and XHwIcap_SelfTest().

u16 XHwIcap_Config::DeviceId

Device ID of device.

int XHwIcap_Config::IcapWidth

Width of ICAP.

Referenced by XHwIcap_CfgInitialize(), XHwIcap_DeviceRead(), and XHwIcap_DeviceWrite().

int XHwIcap_Config::IsLiteMode

IsLiteMode, 0 not present, 1 present.

Referenced by XHwIcap_CfgInitialize().