| uartps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Typedefs | Functions
xuartps_intr.c File Reference

## Typedefs
typedef void(* | Handler )(XUartPs *InstancePtr)
| This function is the handler which performs processing to handle data events from the device. More...

## Functions
u32 | XUartPs_GetInterruptMask (XUartPs *InstancePtr)
| This function gets the interrupt mask. More...
void | XUartPs_SetInterruptMask (XUartPs *InstancePtr, u32 Mask)
| This function sets the interrupt mask. More...
void | XUartPs_SetHandler (XUartPs *InstancePtr, XUartPs_Handler FuncPtr, void *CallBackRef)
| This function sets the handler that will be called when an event (interrupt) occurs that needs application's attention. More...
void | XUartPs_InterruptHandler (XUartPs *InstancePtr)
| This function is the interrupt handler for the driver. More...