| iicps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xiicps_xfer.c File Reference

## Functions
s32 | XIicPs_SetupMaster (XIicPs *InstancePtr, s32 Role)
| This function prepares a device to transfers as a master. More...
void | MasterSendData (XIicPs *InstancePtr)
| This function handles continuation of sending data. More...
void | XIicPs_MasterPolledRead (XIicPs *InstancePtr, s32 IsHold, s32 ByteCountVar)
| Handles polled mode receive in master mode. More...
void | XIicPs_MasterIntrSend (XIicPs *InstancePtr, u32 IntrStatusReg, u32 *StatusEventPtr)
| Handles interrupt-driven send in master mode. More...
void | XIicPs_MasterIntrRead (XIicPs *InstancePtr, u32 *IntrStatusRegPtr, s32 IsHold)
| Handles interrupt-driven receive in master mode. More...
s32 | SlaveRecvData (XIicPs *InstancePtr)
| Handles the continuation of receiving data. More...