| dsi2rx Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xdsi2rx.c File Reference

## Functions
u32 | XDsi2Rx_CfgInitialize (XDsi2Rx *InstancePtr, XDsi2Rx_Config *CfgPtr, UINTPTR EffectiveAddr)
| Initialize the XDsi2Rx instance provided by the caller based on the given Config structure. More...
void | XDsi2Rx_Reset (XDsi2Rx *InstancePtr)
| This function will do a reset of the IP. More...
u32 | XDsi2Rx_DefaultConfigure (XDsi2Rx *InstancePtr)
| This function will configure protocol reg with video mode, Blank packet mode, Blank packet Type, End of Transmisstion packet. More...
u32 | XDsi2Rx_Activate (XDsi2Rx *InstancePtr, XDsi2Rx_Selection Flag)
| This function will enable/disable the IP Core to start processing. More...
void | XDsi2Rx_GetConfigParams (XDsi2Rx *InstancePtr, XDsi2Rx_ConfigParameters *ConfigInfo)
| this function will get the information from the gui settings and other protocol control register values like pixel mode, pixel format. More...