| dfeprach Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfePrach_CCCfg Struct Reference
Overview

Full CC configuration. More...

## Data Fields
XDfePrach_CCSequence | Sequence [XDFEPRACH_BAND_ID_MAX]
       CCID sequence, this needs to match
the CCID sequence generated by the Mixer connected to the PRACH. More...
XDfePrach_InternalCarrierCfg | CarrierCfg [XDFEPRACH_BAND_ID_MAX][XDFEPRACH_CC_NUM_MAX]
                                      Array
of [16] CC configurations More...
u32 | AntennaCfg [XDFEPRACH_ANT_NUM_MAX]
             [0,1] Array of [8] antenna
TDM slot enablement More...

## Detailed Description

Full CC configuration.

## Field Documentation

u32 XDfePrach_CCCfg::AntennaCfg[XDFEPRACH_ANT_NUM_MAX]

             [0,1] Array of [8] antenna

TDM slot enablement

Referenced by XDfePrach_SetAntennaCfgInCCCfg().

XDfePrach_InternalCarrierCfg XDfePrach_CCCfg::CarrierCfg[XDFEPRACH_BAND_ID_MAX][XDFEPRACH_CC_NUM_MAX]

                                      Array

of [16] CC configurations

Referenced by XDfePrach_AddCCtoCCCfgMB(), XDfePrach_GetCarrierCfgMB(), XDfePrach_RemoveCCfromCCCfgMB(), and XDfePrach_UpdateCCinCCCfgMB().

XDfePrach_CCSequence XDfePrach_CCCfg::Sequence[XDFEPRACH_BAND_ID_MAX]

       CCID sequence, this needs to match

the CCID sequence generated by the Mixer connected to the PRACH.

Maximum CC number is 16.

Referenced by XDfePrach_AddCCtoCCCfgMB(), XDfePrach_GetCarrierCfgMB(), XDfePrach_GetEmptyCCCfg(), and XDfePrach_RemoveCCfromCCCfgMB().