| v_frmbuf_rd Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

Data Structures | Macros | Typedefs | Enumerations | Functions
xv_frmbufrd_l2.h File Reference

## Data Structures
struct | XV_FrmbufRd_l2
| Frame Buffer Read driver Layer 2 data. More...

## Macros
#define | XVFrmbufRd_IsRGBX8Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.RGBX8En)
| This macro returns if Video Format RGBX8 is available. More...
#define | XVFrmbufRd_IsYUVX8Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.YUVX8En)
| This macro returns if Video Format YUVX8 is available. More...
#define | XVFrmbufRd_IsY_U_V8Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y_U_V8En)
| This macro returns if Video Format Y_U_V8 is available. More...
#define | XVFrmbufRd_IsY_U_V10Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y_U_V10En)
| This macro returns if Video Format Y_U_V10 is available. More...
#define | XVFrmbufRd_IsY_U_V12Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y_U_V12En)
| This macro returns if Video Format Y_U_V12 is available. More...
#define | XVFrmbufRd_IsY_U_V8_420Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y_U_V8_420En)
| This macro returns if Video Format Y_U_V8_420 is available. More...
#define | XVFrmbufRd_IsYUYV8Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.YUYV8En)
| This macro returns if Video Format YUYV8 is available. More...
#define | XVFrmbufRd_IsRGBA8Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.RGBA8En)
| This macro returns if Video Format RGBA8 is available. More...
#define | XVFrmbufRd_IsYUVA8Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.YUVA8En)
| This macro returns if Video Format YUVA8 is available. More...
#define | XVFrmbufRd_IsRGBX10Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.RGBX10En)
| This macro returns if Video Format RGBX10 is available. More...
#define | XVFrmbufRd_IsYUVX10Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.YUVX10En)
| This macro returns if Video Format YUVX10 is available. More...
#define | XVFrmbufRd_IsY_UV8Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y_UV8En)
| This macro returns if Video Format Y_UV8 is available. More...
#define | XVFrmbufRd_IsY_UV8_420Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y_UV8_420En)
| This macro returns if Video Format Y_UV8_420 is available. More...
#define | XVFrmbufRd_IsRGB8Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.RGB8En)
| This macro returns if Video Format RGB8 is available. More...
#define | XVFrmbufRd_IsYUV8Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.YUV8En)
| This macro returns if Video Format YUV8 is available. More...
#define | XVFrmbufRd_IsY_UV10Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y_UV10En)
| This macro returns if Video Format Y_UV10 is available. More...
#define | XVFrmbufRd_IsY_UV10_420Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y_UV10_420En)
| This macro returns if Video Format Y_UV10_420 is available. More...
#define | XVFrmbufRd_IsY8Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y8En)
| This macro returns if Video Format Y8 is available. More...
#define | XVFrmbufRd_IsY10Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y10En)
| This macro returns if Video Format Y10 is available. More...
#define | XVFrmbufRd_IsBGRA8Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.BGRA8En)
| This macro returns if Video Format BGRA8 is available. More...
#define | XVFrmbufRd_IsBGRX8Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.BGRX8En)
| This macro returns if Video Format BGRX8 is available. More...
#define | XVFrmbufRd_IsUYVY8Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.UYVY8En)
| This macro returns if Video Format UYVY8 is available. More...
#define | XVFrmbufRd_IsBGR8Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.BGR8En)
| This macro returns if Video Format BGR8 is available. More...
#define | XVFrmbufRd_IsRGBX12Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.RGBX12En)
| This macro returns if Video Format RGBX12 is available. More...
#define | XVFrmbufRd_IsRGB16Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.RGB16En)
| This macro returns if Video Format RGB16 is available. More...
#define | XVFrmbufRd_IsYUVX12Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.YUVX12En)
| This macro returns if Video Format YUVX12 is available. More...
#define | XVFrmbufRd_IsYUV16Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.YUV16En)
| This macro returns if Video Format YUV16 is available. More...
#define | XVFrmbufRd_IsY_UV12Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y_UV12En)
| This macro returns if Video Format Y_UV12 is available. More...
#define | XVFrmbufRd_IsY_UV16Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y_UV16En)
| This macro returns if Video Format Y_UV16 is available. More...
#define | XVFrmbufRd_IsY_UV12_420Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y_UV12_420En)
| This macro returns if Video Format Y_UV12_420 is available. More...
#define | XVFrmbufRd_IsY_UV16_420Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y_UV16_420En)
| This macro returns if Video Format Y_UV16_420 is available. More...
#define | XVFrmbufRd_IsY12Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y12En)
| This macro returns if Video Format Y12 is available. More...
#define | XVFrmbufRd_IsY16Enabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Y16En)
| This macro returns if Video Format Y16 is available. More...
#define | XVFrmbufRd_InterlacedEnabled(InstancePtr) ((InstancePtr)->FrmbufRd.Config.Interlaced)
| This macro returns if interlaced support is available. More...

## Typedefs
typedef void(* | XVFrmbufRd_Callback )(void *CallbackRef)
| Callback type for interrupt. More...

## Enumerations
enum | XVFrmbufRd_HandlerType { XVFRMBUFRD_HANDLER_DONE = 1, XVFRMBUFRD_HANDLER_READY }
| These constants specify different types of handler and used to differentiate interrupt requests from peripheral. More...

## Functions
int | XVFrmbufRd_Initialize (XV_FrmbufRd_l2 *InstancePtr, u16 DeviceId)
| This function initializes the core instance. More...
void | XVFrmbufRd_Start (XV_FrmbufRd_l2 *InstancePtr)
| This function starts the core instance. More...
int | XVFrmbufRd_Stop (XV_FrmbufRd_l2 *InstancePtr)
| This function stops the core instance. More...
int | XVFrmbufRd_WaitForIdle (XV_FrmbufRd_l2 *InstancePtr)
| This function Waits for the core to reach idle state. More...
int | XVFrmbufRd_SetMemFormat (XV_FrmbufRd_l2 *InstancePtr, u32 StrideInBytes, XVidC_ColorFormat MemFmt, const XVidC_VideoStream *StrmOut)
| This function configures the frame buffer read memory input. More...
XVidC_VideoStream * | XVFrmbufRd_GetVideoStream (XV_FrmbufRd_l2 *InstancePtr)
| This function reads the pointer to the output stream configuration. More...
int | XVFrmbufRd_SetBufferAddr (XV_FrmbufRd_l2 *InstancePtr, UINTPTR Addr)
| This function sets the buffer address. More...
UINTPTR | XVFrmbufRd_GetBufferAddr (XV_FrmbufRd_l2 *InstancePtr)
| This function reads the buffer address. More...
int | XVFrmbufRd_SetChromaBufferAddr (XV_FrmbufRd_l2 *InstancePtr, UINTPTR Addr)
| This function sets the buffer address for the UV plane for semi-planar formats or Only U Plane for 3 planar formats. More...
UINTPTR | XVFrmbufRd_GetChromaBufferAddr (XV_FrmbufRd_l2 *InstancePtr)
| This function reads the buffer address for the UV plane for semi-planar formats or Only U plane for 3 planar formats. More...
int | XVFrmbufRd_SetVChromaBufferAddr (XV_FrmbufRd_l2 *InstancePtr, UINTPTR Addr)
| This function sets the buffer address for the V plane for 3 planar formats. More...
UINTPTR | XVFrmbufRd_GetVChromaBufferAddr (XV_FrmbufRd_l2 *InstancePtr)
| This function reads the buffer address for the V plane for 3 planar formats. More...
int | XVFrmbufRd_SetFieldID (XV_FrmbufRd_l2 *InstancePtr, u32 FieldID)
| This function sets the field ID. More...
u32 | XVFrmbufRd_GetFieldID (XV_FrmbufRd_l2 *InstancePtr)
| This function reads the field ID. More...
int | XVFrmbufRd_Set_FidOutMode (XV_FrmbufRd_l2 *InstancePtr, u32 fidmodeval)
| This function sets the Fidout Mode Value. More...
u32 | XVFrmbufRd_Get_FidOutMode (XV_FrmbufRd_l2 *InstancePtr)
| This function reads the Fidout Mode Value. More...
u32 | XVFrmbufRd_Get_FidErrorOut (XV_FrmbufRd_l2 *InstancePtr)
| This function reads the Fid error Register and extract error flag. More...
u32 | XVFrmbufRd_Get_FidErrorCount (XV_FrmbufRd_l2 *InstancePtr)
| This function reads the Fid error Register and extract error count. More...
u32 | XVFrmbufRd_Get_FieldOut (XV_FrmbufRd_l2 *InstancePtr)
| This function reads the field Out. More...
void | XVFrmbufRd_DbgReportStatus (XV_FrmbufRd_l2 *InstancePtr)
| This function reports the frame buffer read status. More...
void | XVFrmbufRd_InterruptHandler (void *InstancePtr)
| This function is the interrupt handler for the frame buffer read core driver. More...
int | XVFrmbufRd_SetCallback (XV_FrmbufRd_l2 *InstancePtr, u32 HandlerType, void *CallbackFunc, void *CallbackRef)
| This function installs an asynchronous callback function for the given HandlerType: More...
void | XVFrmbufRd_InterruptEnable (XV_FrmbufRd_l2 *InstancePtr, u32 IrqMask)
| This function enables interrupts in the core. More...
void | XVFrmbufRd_InterruptDisable (XV_FrmbufRd_l2 *InstancePtr, u32 IrqMask)
| This function disables interrupts in the core. More...

## Macro Definition Documentation

#define XVFrmbufRd_InterlacedEnabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Interlaced)

This macro returns if interlaced support is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

#define XVFrmbufRd_IsBGR8Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.BGR8En)

This macro returns if Video Format BGR8 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsBGRA8Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.BGRA8En)

This macro returns if Video Format BGRA8 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsBGRX8Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.BGRX8En)

This macro returns if Video Format BGRX8 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsRGB16Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.RGB16En)

This macro returns if Video Format RGB16 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsRGB8Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.RGB8En)

This macro returns if Video Format RGB8 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsRGBA8Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.RGBA8En)

This macro returns if Video Format RGBA8 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsRGBX10Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.RGBX10En)

This macro returns if Video Format RGBX10 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsRGBX12Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.RGBX12En)

This macro returns if Video Format RGBX12 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsRGBX8Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.RGBX8En)

This macro returns if Video Format RGBX8 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsUYVY8Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.UYVY8En)

This macro returns if Video Format UYVY8 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY10Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y10En)

This macro returns if Video Format Y10 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY12Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y12En)

This macro returns if Video Format Y12 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY16Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y16En)

This macro returns if Video Format Y16 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY8Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y8En)

This macro returns if Video Format Y8 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY_U_V10Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y_U_V10En)

This macro returns if Video Format Y_U_V10 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY_U_V12Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y_U_V12En)

This macro returns if Video Format Y_U_V12 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY_U_V8_420Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y_U_V8_420En)

This macro returns if Video Format Y_U_V8_420 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY_U_V8Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y_U_V8En)

This macro returns if Video Format Y_U_V8 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY_UV10_420Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y_UV10_420En)

This macro returns if Video Format Y_UV10_420 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY_UV10Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y_UV10En)

This macro returns if Video Format Y_UV10 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY_UV12_420Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y_UV12_420En)

This macro returns if Video Format Y_UV12_420 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY_UV12Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y_UV12En)

This macro returns if Video Format Y_UV12 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY_UV16_420Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y_UV16_420En)

This macro returns if Video Format Y_UV16_420 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY_UV16Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y_UV16En)

This macro returns if Video Format Y_UV16 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY_UV8_420Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y_UV8_420En)

This macro returns if Video Format Y_UV8_420 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsY_UV8Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.Y_UV8En)

This macro returns if Video Format Y_UV8 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsYUV16Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.YUV16En)

This macro returns if Video Format YUV16 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsYUV8Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.YUV8En)

This macro returns if Video Format YUV8 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsYUVA8Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.YUVA8En)

This macro returns if Video Format YUVA8 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsYUVX10Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.YUVX10En)

This macro returns if Video Format YUVX10 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsYUVX12Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.YUVX12En)

This macro returns if Video Format YUVX12 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsYUVX8Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.YUVX8En)

This macro returns if Video Format YUVX8 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

#define XVFrmbufRd_IsYUYV8Enabled | ( |  | InstancePtr | ) | ((InstancePtr)->FrmbufRd.Config.YUYV8En)

This macro returns if Video Format YUYV8 is available.

Parameters

  InstancePtr | is a pointer to the core instance.

Returns
  Enabled(1)/Disabled(0)

Note
  None.

Referenced by XVFrmbufRd_SetMemFormat().

## Typedef Documentation

typedef void(* XVFrmbufRd_Callback)(void *CallbackRef)

Callback type for interrupt.

Parameters

  CallbackRef | is a callback reference passed in by the upper layer when setting the callback functions, and passed back to the upper layer when the callback is invoked.

Returns
  None.

Note
  None.