| dfeofdm Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfeOfdm_TriggerCfg Struct Reference
Overview

All IP triggers. More...

## Data Fields
XDfeOfdm_Trigger | Activate
                        Switch between "Initialized",
ultra-low power state, and "Operational". More...
XDfeOfdm_Trigger | LowPower
                        Switch between "Low-power"
and "Operational" state. More...
XDfeOfdm_Trigger | CCUpdate
                        Transition to next CC
configuration. More...

## Detailed Description

All IP triggers.

## Field Documentation

XDfeOfdm_Trigger XDfeOfdm_TriggerCfg::Activate

                        Switch between "Initialized",

ultra-low power state, and "Operational".

One-shot trigger, disabled following a single event.

Referenced by XDfeOfdm_AddCCExample(), XDfeOfdm_GetTriggersCfg(), XDfeOfdm_MultiAddCCExample(), and XDfeOfdm_SetTriggersCfg().

XDfeOfdm_Trigger XDfeOfdm_TriggerCfg::CCUpdate

                        Transition to next CC

configuration.

Will initiate flush based on CC configuration.

Referenced by XDfeOfdm_AddCCExample(), XDfeOfdm_GetTriggersCfg(), XDfeOfdm_MultiAddCCExample(), and XDfeOfdm_SetTriggersCfg().

XDfeOfdm_Trigger XDfeOfdm_TriggerCfg::LowPower

                        Switch between "Low-power"

and "Operational" state.

Referenced by XDfeOfdm_GetTriggersCfg(), and XDfeOfdm_SetTriggersCfg().