| v_hdmiphy1 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XHdmiphy1_Log Struct Reference
Overview

This typedef contains the logging mechanism for debug. More...

## Data Fields
u16 | DataBuffer [128]
| Log buffer with event data. More...
u64 | TimeRecord [128]
| Log time for the event. More...
u8 | HeadIndex
         Index of the head entry of the
Event/DataBuffer. More...
u8 | TailIndex
         Index of the tail entry of the
Event/DataBuffer. More...

## Detailed Description

This typedef contains the logging mechanism for debug.

## Field Documentation

u16 XHdmiphy1_Log::DataBuffer[128]

Log buffer with event data.

Referenced by XHdmiphy1_LogRead(), and XHdmiphy1_LogWrite().

u8 XHdmiphy1_Log::HeadIndex

         Index of the head entry of the

Event/DataBuffer.

Referenced by XHdmiphy1_LogRead(), XHdmiphy1_LogReset(), and XHdmiphy1_LogWrite().

u8 XHdmiphy1_Log::TailIndex

         Index of the tail entry of the

Event/DataBuffer.

Referenced by XHdmiphy1_LogDisplay(), XHdmiphy1_LogRead(), XHdmiphy1_LogReset(), and XHdmiphy1_LogWrite().

u64 XHdmiphy1_Log::TimeRecord[128]

Log time for the event.

Referenced by XHdmiphy1_LogDisplay(), and XHdmiphy1_LogWrite().