| dmaps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDmaPs_Config Struct Reference
Overview

This typedef contains configuration information for the device. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
u32 | BaseAddress
| Base address of device (IPIF) More...

## Detailed Description

This typedef contains configuration information for the device.

## Field Documentation

u32 XDmaPs_Config::BaseAddress

Base address of device (IPIF)

Referenced by XDmaPs_CfgInitialize(), XDmaPs_FaultISR(), XDmaPs_ResetChannel(), XDmaPs_ResetManager(), XDmaPs_SelfTest(), and XDmaPs_Start().

u16 XDmaPs_Config::DeviceId

Unique ID of device.

Referenced by XDmaPs_CfgInitialize(), and XDmaPs_FaultISR().