| iomodule Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Data Structures | Macros | Functions
xiomodule_l.h File Reference

## Data Structures
struct | XIOModule_VectorTableEntry
| Defines the number of timer counters within a single hardware device. More...

## Macros
#define | XIOModule_EnableIntr(BaseAddress, EnableMask) XIomodule_Out32((BaseAddress) + XIN_IER_OFFSET, (EnableMask))
| Enable specific interrupt(s) in the interrupt controller. More...
#define | XIOModule_DisableIntr(BaseAddress, DisableMask) XIomodule_Out32((BaseAddress) + XIN_IER_OFFSET, ~(DisableMask))
| Disable specific interrupt(s) in the interrupt controller. More...
#define | XIOModule_AckIntr(BaseAddress, AckMask) XIomodule_Out32((BaseAddress) + XIN_IAR_OFFSET, (AckMask))
| Acknowledge specific interrupt(s) in the interrupt controller. More...
#define | XIOModule_GetIntrStatus(BaseAddress) (XIomodule_In32((BaseAddress) + XIN_IPR_OFFSET))
| Get the interrupt status from the interrupt controller which indicates which interrupts are active and enabled. More...
#define | XIOModule_GetStatusReg(BaseAddress) XIomodule_In32((BaseAddress) + XUL_STATUS_REG_OFFSET)
| Get the contents of the UART status register. More...
#define | XIOModule_IsReceiveEmpty(BaseAddress)
| Check to see if the UART receiver has data. More...
#define | XIOModule_IsTransmitFull(BaseAddress)
| Check to see if the transmitter is full. More...
#define | XIOModule_WriteReg(BaseAddress, RegOffset, Data) XIomodule_Out32((BaseAddress) + (RegOffset), (u32)(Data))
| Write a value to a GPO register. More...
#define | XIOModule_ReadReg(BaseAddress, RegOffset) XIomodule_In32((BaseAddress) + (RegOffset))
| Read a value from a GPI register. More...

## Functions
void | XIOModule_SendByte (UINTPTR BaseAddress, u8 Data)
| This functions sends a single byte using the UART. More...
u8 | XIOModule_RecvByte (UINTPTR BaseAddress)
| This functions receives a single byte using the UART. More...
void | XIOModule_DeviceInterruptHandler (void *DeviceId)
| This function is the primary interrupt handler for the driver. More...
void | XIOModule_SetIntrSvcOption (UINTPTR BaseAddress, s32 Option)
| Set the interrupt service option, which can configure the driver so that it services only a single interrupt at a time when an interrupt occurs, or services all pending interrupts when an interrupt occurs. More...
void | XIOModule_RegisterHandler (UINTPTR BaseAddress, s32 InterruptId, XInterruptHandler Handler, void *CallBackRef)
| Register a handler function for a specific interrupt ID. More...