| v_hdmirxss1 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
Overview

## Functions
int | XV_HdmiRxSs1_SubcoreInitHdmiRx1 (XV_HdmiRxSs1 *HdmiRxSs1Ptr)
| This function initializes the included sub-core to it's static configuration. More...
XV_HdmiRxSs1_Config * | XV_HdmiRxSs1_LookupConfig (u32 DeviceId)
| This function looks for the device configuration based on the unique device ID. More...

## Function Documentation

XV_HdmiRxSs1_Config* XV_HdmiRxSs1_LookupConfig | ( | u32 | DeviceId | ) |

This function looks for the device configuration based on the unique device ID.

The table XV_HdmiRxSs1_ConfigTable[] contains the configuration information for each instance of the device in the system.

Parameters

  DeviceId | is the unique device ID of the device being looked up

Returns
  A pointer to the configuration table entry corresponding to the given device ID, or NULL if no match is found

int XV_HdmiRxSs1_SubcoreInitHdmiRx1 | ( | XV_HdmiRxSs1 * | HdmiRxSs1Ptr | ) |

This function initializes the included sub-core to it's static configuration.

Parameters

  HdmiRxSs1Ptr | is a pointer to the Subsystem instance to be worked on.

Returns
  XST_SUCCESS/XST_FAILURE

References XV_HdmiRxSs1_SubCore::AbsAddr, XV_HdmiRxSs1_Config::AxiLiteClkFreq, XV_HdmiRxSs1_Config::BaseAddress, XV_HdmiRxSs1::Config, XV_HdmiRxSs1_SubCore::DeviceId, XV_HdmiRxSs1::EdidLength, XV_HdmiRxSs1::EdidPtr, XV_HdmiRxSs1_Config::HdmiRx1, XV_HdmiRxSs1::HdmiRx1Ptr, XV_HdmiRxSs1_Config::Ppc, XV_HdmiRxSs1_Config::VideoInterface, XV_HDMIRXSS1_LOG_EVT_HDMIRX1_INIT, and XV_HdmiRxSs1_LogWrite().

Referenced by XV_HdmiRxSs1_CfgInitialize().