| dfeccf Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfeCcf_CCSequence Struct Reference
Overview

Defines a CCID sequence. More...

## Data Fields
u32 | Length
| [1-16] Sequence length. More...
s32 | CCID [XDFECCF_SEQ_LENGTH_MAX]
       [0-15].Array of CCID's
arranged in the order the CCIDs are required to be processed in the channel filter. More...
s32 | NotUsedCCID
| Lowest CCID number not allocated. More...

## Detailed Description

Defines a CCID sequence.

## Field Documentation

s32 XDfeCcf_CCSequence::CCID[XDFECCF_SEQ_LENGTH_MAX]

       [0-15].Array of CCID's

arranged in the order the CCIDs are required to be processed in the channel filter.

Referenced by XDfeCcf_GetCarrierCfg(), and XDfeCcf_GetEmptyCCCfg().

u32 XDfeCcf_CCSequence::Length

[1-16] Sequence length.

Referenced by XDfeCcf_AddCC(), XDfeCcf_GetCarrierCfg(), XDfeCcf_GetEmptyCCCfg(), XDfeCcf_Initialize(), and XDfeCcf_PassThroughExample().

s32 XDfeCcf_CCSequence::NotUsedCCID

Lowest CCID number not allocated.

Referenced by XDfeCcf_GetCurrentCCCfg(), XDfeCcf_GetCurrentCCCfgSwitchable(), XDfeCcf_SetNextCCCfgAndTrigger(), and XDfeCcf_SetNextCCCfgAndTriggerSwitchable().