| v_hdmitxss Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Macros | Functions | Variables
xv_hdmitxss.c File Reference

## Overview

This is main code of Xilinx HDMI Transmitter Subsystem device driver.

Please see xv_hdmitxss.h for more details of the driver.

    MODIFICATION HISTORY:

    Ver   Who    Date     Changes

    1.00         10/07/15 Initial release.
    1.01  MG     17/12/16 Fixed issue in function SetAudioChannels
                          Updated function XV_HdmiTxSs_SendAuxInfoframe
    1.02  yh     12/01/16 Check vtc existance before configuring it
    1.03  yh     15/01/16 Add 3D Support
    1.04  yh     20/01/16 Added remapper support
    1.05  yh     01/02/16 Added set_ppc api
    1.06  yh     01/02/16 Removed xil_print "Cable (dis)connected"
    1.07  yh     15/02/16 Added default value to XV_HdmiTxSs_ConfigRemapper
    1.08  MG     03/02/16 Added HDCP support
    1.09  MG     09/03/16 Added XV_HdmiTxSs_SetHdmiMode and XV_HdmiTxSs_SetDviMode
                          Removed reduced blanking support
    1.10  MH     03/15/16 Moved HDCP 2.2 reset from stream up/down callback to
                          connect callback
    1.11  YH     18/03/16 Add XV_HdmiTxSs_SendGenericAuxInfoframe function
    1.12  MH     23/04/16 1. HDCP 1.x driver now uses AXI timer 4.1, so updated
                          to use AXI Timer config structure to determine timer
                          clock frequency
                          2. HDCP 1.x driver has fixed the problem where the
                          reset for the receiver causes the entire DDC peripheral
                          to get reset. Based on this change the driver has been
                          updated to use XV_HdmiTxSs_HdcpReset and
                          XV_HdmiTxSs_HdcpReset functions directly.
                          3. Updated XV_HdmiTxSs_HdcpEnable and
                          XV_HdmiTxSs_HdcpEnable functions to ensure that
                          HDCP 1.4 and 2.2 are mutually exclusive.
                          This fixes the problem where HDCP 1.4 and 2.2
                          state machines are running simultaneously.
    1.13   MH    23/06/16 Added HDCP repeater support.
    1.14   YH    18/07/16 1. Replace xil_print with xdbg_printf.
                          2. XV_HdmiTx_VSIF VSIF global variable local to
                           XV_HdmiTxSs_SendVSInfoframe
                          3. Replace MB_Sleep() with usleep
                          4. Remove checking VideoMode < XVIDC_VM_NUM_SUPPORTED in
                          XV_HdmiTxSs_SetStream to support customized video format
    1.15   YH    25/07/16 Used UINTPTR instead of u32 for BaseAddress
                          XV_HdmiTxSs_CfgInitialize
    1.16   YH    04/08/16 Remove unused functions
                          XV_HdmiTxSs_GetSubSysStruct
    1.17   MH    08/08/16 Updates to optimize out HDCP when excluded.
    1.18   YH    17/08/16 Remove sleep in XV_HdmiTxSs_ResetRemapper
                          Added Event Log
                          Combine Report function into one ReportInfo
    1.19   YH    27/08/16 Remove unused functions XV_HdmiTxSs_SetUserTimerHandler
                          XV_HdmiTxSs_WaitUs
    1.20   MH    08/10/16 Update function call sequence in
                          XV_HdmiTxSs_StreamUpCallback

    1.1x   mmo   04/11/16 Updated the XV_HdmiTxSs_SetAudioChannels API which
                          currently calls XV_HdmiTx_SetAudioChannels driver,
                          which sets the Audio Channels
                          accordingly. This fixed is made during v1.2 (2016.1)
    1.21  YH     14/11/16 Added API to enable/disable YUV420/Pixel Repeat Mode
                          for video bridge
    1.22  YH     14/11/16 Remove Remapper APIs as remapper feature is moved to
                          video bridge and controlled by HDMI core
    1.23  mmo    03/01/17 Move HDCP Related API to xv_hdmitxss_hdcp.c
                          Remove inclusion of the xenv.h and sleep.h as it not
                              used
                          Replaced "print" with "xil_printf"
                          Replace Carriage Return () and Line Feed (

    ) order,\
                              where the Carriage Return + Line Feed order is used.
    1.24  mmo    02/03/17 Added XV_HdmiTxSs_ReadEdidSegment API for Multiple
                                Segment Support and HDMI Compliance Test
                          Updated the XV_HdmiTxSs_ShowEdid API to have support
                                multiple EDID.
    1.25  MH     21/04/17 Updated to set HDMI mode in functions
                                XV_HdmiTxSS_SetHdmiMode and XV_HdmiTxSS_SetDviMode.
    1.40  YH     07/07/17 Fixed issue with VTC register read when video clock is
                                not present
                          Report HDMI/DVI mode in HDMI example design info log
                          Added Video Masking APIs
    1.41  mmo    02/08/17 Initialize the hdcp1.4 first before the hdcp1.4 timer
                                 as the hdcp1.4 timer requires hdcp1.4 to be
                                 initialize
          MH     09/08/17 Added function XV_HdmiTxSs_HdcpSetCapability
                 22/08/17 Added function XV_HdmiTxSs_SetAudioFormat
    1.42  YH     06/10/17 Updated function XV_HdmiTxSs_SetAudioFormat
                          Added function XV_HdmiTxSs_GetAudioFormat
          EB     17/10/17 Added function XV_HdmiTxSs_ReportAudio
                          Updated function XV_HdmiTxSs_ReportInfo
    1.43  MMO    19/12/17 Added XV_HdmiTxSS_SetTMDS API
    5.00  EB     16/01/18 Updated XV_HdmiTxSS_SetTMDS API
                          Updated XV_HdmiTxSs_SetVideoStream API
                          Moved XV_HdmiTxSs_SendVSInfoframe function to HDMI
                                                        Common Library
                          Updated function XV_HdmiTxSs_StreamStart,
                                  XV_HdmiTxSs_SendGenericAuxInfoframe
                          Added function XV_HdmiTxSs_GetAviInfoframe,
                              XV_HdmiTxSs_GetAudioInfoframe, XV_HdmiTxSs_GetVSIF
                              XV_HdmiTxSs_GetAuxiliary
                          Updated XV_HdmiTxSs_ConfigBridgeMode so Pixel
                              Pepetition AVI InfoFrame is sent out
                          Deprecating XV_HdmiTxSs_SendAviInfoframe and
                              XV_HdmiTxSs_SendGeneralControlPacket APIs
          YH     16/01/18 Added dedicated reset for each clock domain
                          Added bridge unlock interrupt
                          Added PIO_OUT to set GCP_AVMUTE
          EB     23/01/18 Added function
                              XV_HdmiTxSs_SetVideoStreamHdmi14ScramblingOverrideFlag
                 25/01/18 Added function XV_HdmiTxSs_SetScrambler
                 01/02/18   Updated function XV_HdmiTxSs_VtcSetup and changed the
                              input parameters to it to enable logging of
                              unsupported video timing by VTC
          SM     28/02/18 Added definition of XV_HdmiTxSS_SetAppVersion() API
    5.20  EB     03/08/18 Updated XV_HdmiTxSS_MaskSetRed, XV_HdmiTxSS_MaskSetGreen,
                              XV_HdmiTxSS_MaskSetBlue API
                          Replaced XV_HdmiTx_AudioMute API call with
                              XV_HdmiTx_AudioDisable
                          Replaced XV_HdmiTx_AudioUnmute API call with
                              XV_HdmiTx_AudioEnable
                          Replaced XV_HdmiTx_AudioUnmute API call with
                    MMO    11/08/18 Added Bridge Overflow and Bridge Underflow Interrupt

## Macros
#define | XV_HdmiTxSs_BridgeYuv420(InstancePtr, Enable)
| This macro selects the bridge YUV420 mode. More...
#define | XV_HdmiTxSs_BridgePixelRepeat(InstancePtr, Enable)
| This macro selects the bridge pixel repeat mode. More...

## Functions
void | XV_HdmiTxSS_SetHdmiMode (XV_HdmiTxSs *InstancePtr)
| This function sets the core into HDMI mode. More...
void | XV_HdmiTxSS_SetDviMode (XV_HdmiTxSs *InstancePtr)
| This function sets the core into DVI mode. More...
void | XV_HdmiTxSS_HdmiTxIntrHandler (XV_HdmiTxSs *InstancePtr)
| This function calls the interrupt handler for HDMI TX. More...
int | XV_HdmiTxSs_CfgInitialize (XV_HdmiTxSs *InstancePtr, XV_HdmiTxSs_Config *CfgPtr, UINTPTR EffectiveAddr)
| This function initializes the video subsystem and included sub-cores. More...
void | XV_HdmiTxSs_Start (XV_HdmiTxSs *InstancePtr)
| This function starts the HDMI TX subsystem including all sub-cores that are included in the processing pipeline for a given use-case. More...
void | XV_HdmiTxSs_Stop (XV_HdmiTxSs *InstancePtr)
| This function stops the HDMI TX subsystem including all sub-cores Stop the video pipe starting from front to back. More...
void | XV_HdmiTxSs_Reset (XV_HdmiTxSs *InstancePtr)
| This function resets the video subsystem sub-cores. More...
void | XV_HdmiTxSs_TXCore_VRST (XV_HdmiTxSs *InstancePtr, u8 Reset)
| This function asserts or releases the Internal Video reset of the HDMI subcore within the subsystem. More...
void | XV_HdmiTxSs_TXCore_LRST (XV_HdmiTxSs *InstancePtr, u8 Reset)
| This function asserts or releases the Internal Link reset of the HDMI subcore within the subsystem. More...
void | XV_HdmiTxSs_VRST (XV_HdmiTxSs *InstancePtr, u8 Reset)
| This function asserts or releases the video reset of other blocks within the subsystem. More...
void | XV_HdmiTxSs_SYSRST (XV_HdmiTxSs *InstancePtr, u8 Reset)
| This function asserts or releases the system reset of other blocks within the subsystem. More...
void | XV_HdmiTxSs_SetGcpAvmuteBit (XV_HdmiTxSs *InstancePtr)
| This function sets the HDMI TX AUX GCP register AVMUTE bit. More...
void | XV_HdmiTxSs_ClearGcpAvmuteBit (XV_HdmiTxSs *InstancePtr)
| This function clears the HDMI TX AUX GCP register AVMUTE bit. More...
void | XV_HdmiTxSs_SetGcpClearAvmuteBit (XV_HdmiTxSs *InstancePtr)
| This function sets the HDMI TX AUX GCP register CLEAR_AVMUTE bit. More...
void | XV_HdmiTxSs_ClearGcpClearAvmuteBit (XV_HdmiTxSs *InstancePtr)
| This function clears the HDMI TX AUX GCP register CLEAR_AVMUTE bit. More...
int | XV_HdmiTxSs_SetCallback (XV_HdmiTxSs *InstancePtr, XV_HdmiTxSs_HandlerType HandlerType, void *CallbackFunc, void *CallbackRef)
| This function installs an asynchronous callback function for the given HandlerType: More...
int | XV_HdmiTxSs_ReadEdid (XV_HdmiTxSs *InstancePtr, u8 *Buffer)
| This function reads the HDMI Sink EDID. More...
int | XV_HdmiTxSs_ReadEdidSegment (XV_HdmiTxSs *InstancePtr, u8 *Buffer, u8 segment)
| This function reads one block from the HDMI Sink EDID. More...
void | XV_HdmiTxSs_ShowEdid (XV_HdmiTxSs *InstancePtr)
| This function shows the HDMI source edid. More...
void | XV_HdmiTxSs_StreamStart (XV_HdmiTxSs *InstancePtr)
| This function starts the HDMI TX stream. More...
void | XV_HdmiTxSs_SetScrambler (XV_HdmiTxSs *InstancePtr, u8 Enable)
| This function enables / disables the TX scrambler. More...
void | XV_HdmiTxSs_SendAuxInfoframe (XV_HdmiTxSs *InstancePtr, void *Aux)
| This function sends audio info frames. More...
u32 | XV_HdmiTxSs_SendGenericAuxInfoframe (XV_HdmiTxSs *InstancePtr, void *Aux)
| This function sends generic info frames. More...
void | XV_HdmiTxSs_SetAudioChannels (XV_HdmiTxSs *InstancePtr, u8 AudioChannels)
| This function Sets the HDMI TX SS number of active audio channels. More...
void | XV_HdmiTxSs_AudioMute (XV_HdmiTxSs *InstancePtr, u8 Enable)
| This function set HDMI TX audio parameters. More...
void | XV_HdmiTxSs_SetAudioFormat (XV_HdmiTxSs *InstancePtr, XV_HdmiTx_AudioFormatType format)
| This function Sets the HDMI TX SS Audio Format. More...
XV_HdmiTx_AudioFormatType | XV_HdmiTxSs_GetAudioFormat (XV_HdmiTxSs *InstancePtr)
| This function gets the active audio format. More...
XHdmiC_Aux * | XV_HdmiTxSs_GetAuxiliary (XV_HdmiTxSs *InstancePtr)
| This function returns the pointer to HDMI TX SS Aux structure. More...
XHdmiC_AVI_InfoFrame * | XV_HdmiTxSs_GetAviInfoframe (XV_HdmiTxSs *InstancePtr)
| This function returns the pointer to HDMI TX SS AVI InfoFrame structure. More...
XHdmiC_AudioInfoFrame * | XV_HdmiTxSs_GetAudioInfoframe (XV_HdmiTxSs *InstancePtr)
| This function returns the pointer to HDMI TX SS Audio InfoFrame structure. More...
XHdmiC_VSIF * | XV_HdmiTxSs_GetVSIF (XV_HdmiTxSs *InstancePtr)
| This function returns the pointer to HDMI TX SS Vendor Specific InfoFrame structure. More...
XHdmiC_DRMInfoFrame * | XV_HdmiTxSs_GetDrmInfoframe (XV_HdmiTxSs *InstancePtr)
| This function returns the pointer to HDMI TX SS DRM InfoFrame structure. More...
u32 | XV_HdmiTxSs_SetStream (XV_HdmiTxSs *InstancePtr, XVidC_VideoMode VideoMode, XVidC_ColorFormat ColorFormat, XVidC_ColorDepth Bpc, XVidC_3DInfo *Info3D)
| This function set HDMI TX susbsystem stream parameters. More...
XVidC_VideoStream * | XV_HdmiTxSs_GetVideoStream (XV_HdmiTxSs *InstancePtr)
| This function returns the pointer to HDMI TX SS video stream. More...
void | XV_HdmiTxSs_SetVideoStream (XV_HdmiTxSs *InstancePtr, XVidC_VideoStream VidStream)
| This function Sets the HDMI TX SS video stream. More...
void | XV_HdmiTxSs_SetSamplingRate (XV_HdmiTxSs *InstancePtr, u8 SamplingRate)
| This function Sets the HDMI TX SS video Identification code. More...
void | XV_HdmiTxSs_SetVideoIDCode (XV_HdmiTxSs *InstancePtr, u8 Vic)
| This function Sets the HDMI TX SS video Identification code. More...
void | XV_HdmiTxSs_SetVideoStreamType (XV_HdmiTxSs *InstancePtr, u8 StreamType)
| This function Sets the HDMI TX SS video stream type. More...
void | XV_HdmiTxSs_SetVideoStreamScramblingFlag (XV_HdmiTxSs *InstancePtr, u8 IsScrambled)
| This function Sets the HDMI TX SS video stream type. More...
void | XV_HdmiTxSs_SetVideoStreamScramblingOverrideFlag (XV_HdmiTxSs *InstancePtr, u8 OverrideScramble)
| This function Sets the HDMI TX SS video stream scrambling behaviour. More...
void | XV_HdmiTxSs_SetTmdsClockRatio (XV_HdmiTxSs *InstancePtr, u8 Ratio)
| This function Sets the HDMI TX SS TMDS Cock Ratio. More...
u32 | XV_HdmiTxSs_GetTmdsClockFreqHz (XV_HdmiTxSs *InstancePtr)
| This function Sets the HDMI TX SS video Identification code. More...
int | XV_HdmiTxSs_DetectHdmi20 (XV_HdmiTxSs *InstancePtr)
| This function detects connected sink is a HDMI 2.0/HDMI 1.4 sink device. More...
void | XV_HdmiTxSs_RefClockChangeInit (XV_HdmiTxSs *InstancePtr)
| This function is called when HDMI TX SS TMDS clock changes. More...
void | XV_HdmiTxSs_ReportInfo (XV_HdmiTxSs *InstancePtr)
| This function prints the HDMI TX SS subcore versions. More...
int | XV_HdmiTxSs_IsStreamUp (XV_HdmiTxSs *InstancePtr)
| This function checks if the video stream is up. More...
int | XV_HdmiTxSs_IsStreamConnected (XV_HdmiTxSs *InstancePtr)
| This function checks if the interface is connected. More...
int | XV_HdmiTxSs_IsStreamToggled (XV_HdmiTxSs *InstancePtr)
| This function checks if the interface has toggled. More...
void | XV_HdmiTxSs_SetDefaultPpc (XV_HdmiTxSs *InstancePtr, u8 Id)
| This function will set the default in HDF. More...
void | XV_HdmiTxSs_SetPpc (XV_HdmiTxSs *InstancePtr, u8 Id, u8 Ppc)
| This function will set PPC specified by user. More...
void | XV_HdmiTxSS_MaskEnable (XV_HdmiTxSs *InstancePtr)
| This function will enable the video masking. More...
void | XV_HdmiTxSS_MaskDisable (XV_HdmiTxSs *InstancePtr)
| This function will disable the video masking. More...
void | XV_HdmiTxSS_MaskNoise (XV_HdmiTxSs *InstancePtr, u8 Enable)
| This function will enable or disable the noise in the video mask. More...
void | XV_HdmiTxSS_MaskSetRed (XV_HdmiTxSs *InstancePtr, u16 Value)
| This function will set the red component in the video mask. More...
void | XV_HdmiTxSS_MaskSetGreen (XV_HdmiTxSs *InstancePtr, u16 Value)
| This function will set the green component in the video mask. More...
void | XV_HdmiTxSS_MaskSetBlue (XV_HdmiTxSs *InstancePtr, u16 Value)
| This function will set the blue component in the video mask. More...
void | XV_HdmiTxSS_SetBackgroundColor (XV_HdmiTxSs *InstancePtr, XVMaskColorId ColorId)
| This function configures the background color for Video Masking Feature. More...
u8 | XV_HdmiTxSS_IsMasked (XV_HdmiTxSs *InstancePtr)
| This function will get the current video mask mode. More...
void | XV_HdmiTxSS_SetAppVersion (XV_HdmiTxSs *InstancePtr, u8 maj, u8 min)
| This function will set the major and minor application version in TXSs struct. More...
void | XV_HdmiTxSS_SetHpdTolerance (XV_HdmiTxSs *InstancePtr, XV_HdmiTxSs_HpdToleranceType Type, u16 ToleranceVal)
| This function will Configure Timegrid based on the tolerance value for HPD and Toggle event. More...

## Variables
XV_HdmiTxSs_SubCores | XV_HdmiTxSs_SubCoreRepo [XPAR_XV_HDMITXSS_NUM_INSTANCES]
| Define Driver instance of all sub-core included in the design. More...

## Macro Definition Documentation

#define XV_HdmiTxSs_BridgePixelRepeat | ( |  | InstancePtr,
|  |  | Enable
| ) |  |

Value:
{ \
XV_HdmiTx_Bridge_pixel(InstancePtr->HdmiTxPtr, Enable); \
}

This macro selects the bridge pixel repeat mode.

Parameters

  InstancePtr | is a pointer to the HDMI TX Subsystem

#define XV_HdmiTxSs_BridgeYuv420 | ( |  | InstancePtr,
|  |  | Enable
| ) |  |

Value:
{ \
XV_HdmiTx_Bridge_yuv420(InstancePtr->HdmiTxPtr, Enable); \
}

This macro selects the bridge YUV420 mode.

Parameters

  InstancePtr | is a pointer to the HDMI TX Subsystem

## Function Documentation

void XV_HdmiTxSs_AudioMute | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | Enable
| ) |  |

This function set HDMI TX audio parameters.

Parameters

  Enable | 0: Unmute the audio 1: Mute the audio.

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr, XV_HDMITXSS_LOG_EVT_AUDIOMUTE, XV_HDMITXSS_LOG_EVT_AUDIOUNMUTE, and XV_HdmiTxSs_LogWrite().

Referenced by XV_HdmiTxSs_SetVideoStreamType().

int XV_HdmiTxSs_CfgInitialize | ( | XV_HdmiTxSs * | InstancePtr,
|  | XV_HdmiTxSs_Config * | CfgPtr,
|  | UINTPTR | EffectiveAddr
| ) |  |

This function initializes the video subsystem and included sub-cores.

This function must be called prior to using the subsystem. Initialization includes setting up the instance data for top level as well as all included sub-core therein, and ensuring the hardware is in a known stable state.

Parameters

  InstancePtr | is a pointer to the Subsystem instance to be worked on.
  CfgPtr | points to the configuration structure associated with the subsystem instance.
  EffectiveAddr | is the base address of the device. If address translation is being used, then this parameter must reflect the virtual base address. Otherwise, the physical address should be used.

Returns
  XST_SUCCESS if initialization is successful else XST_FAILURE

References XV_HdmiTxSs::AppMajVer, XV_HdmiTxSs::AppMinVer, XV_HdmiTxSs::AudioInfoframe, XV_HdmiTxSs::AVIInfoframe, XV_HdmiTxSs_Config::AxiLiteClkFreq, XV_HdmiTxSs_Config::BaseAddress, XV_HdmiTxSs::Config, XV_HdmiTxSs_Config::DeviceId, XV_HdmiTxSs::DrmInfoframe, XV_HdmiTxSs::HdcpProtocol, XV_HdmiTxSs::HdmiTxPtr, XV_HdmiTxSs::IsReady, XV_HdmiTxSs::VSIF, XV_HdmiTxSs::VtcPtr, XV_HDMITXSS_HDCP_BOTH, XV_HDMITXSS_HDCP_NONE, XV_HdmiTxSs_Reset(), XV_HdmiTxSs_SubcoreInitHdmiTx(), and XV_HdmiTxSs_SubcoreInitVtc().

void XV_HdmiTxSs_ClearGcpAvmuteBit | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function clears the HDMI TX AUX GCP register AVMUTE bit.

Parameters

  InstancePtr | is a pointer to the Subsystem instance to be worked on.

Returns
  None

References XV_HdmiTxSs::HdmiTxPtr.

void XV_HdmiTxSs_ClearGcpClearAvmuteBit | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function clears the HDMI TX AUX GCP register CLEAR_AVMUTE bit.

Parameters

  InstancePtr | is a pointer to the Subsystem instance to be worked on.

Returns
  None

References XV_HdmiTxSs::HdmiTxPtr.

int XV_HdmiTxSs_DetectHdmi20 | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function detects connected sink is a HDMI 2.0/HDMI 1.4 sink device.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTxSs core instance.

Returns
  - XST_SUCCESS if HDMI 2.0
  - XST_FAILURE if HDMI 1.4

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

XV_HdmiTx_AudioFormatType XV_HdmiTxSs_GetAudioFormat | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function gets the active audio format.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTxSs core instance.

Returns
  Active audio format of HDMI Tx Subsystem

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

XHdmiC_AudioInfoFrame* XV_HdmiTxSs_GetAudioInfoframe | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function returns the pointer to HDMI TX SS Audio InfoFrame structure.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance

Returns
  XHdmiC_AudioInfoFrame pointer

Note
  None.

References XV_HdmiTxSs::AudioInfoframe.

XHdmiC_Aux* XV_HdmiTxSs_GetAuxiliary | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function returns the pointer to HDMI TX SS Aux structure.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance

Returns
  XVidC_VideoStream pointer

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

XHdmiC_AVI_InfoFrame* XV_HdmiTxSs_GetAviInfoframe | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function returns the pointer to HDMI TX SS AVI InfoFrame structure.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance

Returns
  XHdmiC_AVI_InfoFrame pointer

Note
  None.

References XV_HdmiTxSs::AVIInfoframe.

XHdmiC_DRMInfoFrame* XV_HdmiTxSs_GetDrmInfoframe | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function returns the pointer to HDMI TX SS DRM InfoFrame structure.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance

Returns
  XHdmiC_DRMInfoFrame pointer

Note
  None.

References XV_HdmiTxSs::DrmInfoframe.

u32 XV_HdmiTxSs_GetTmdsClockFreqHz | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function Sets the HDMI TX SS video Identification code.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance
  @return | Stream Data Structure (TMDS Clock)

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

XVidC_VideoStream* XV_HdmiTxSs_GetVideoStream | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function returns the pointer to HDMI TX SS video stream.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance

Returns
  XVidC_VideoStream pointer

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

Referenced by XV_HdmiTxSS_SetBackgroundColor().

XHdmiC_VSIF* XV_HdmiTxSs_GetVSIF | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function returns the pointer to HDMI TX SS Vendor Specific InfoFrame structure.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance

Returns
  XHdmiC_VSIF pointer

Note
  None.

References XV_HdmiTxSs::VSIF.

void XV_HdmiTxSS_HdmiTxIntrHandler | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function calls the interrupt handler for HDMI TX.

Parameters

  InstancePtr | is a pointer to the HDMI TX Subsystem

References XV_HdmiTxSs::HdmiTxPtr.

u8 XV_HdmiTxSS_IsMasked | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function will get the current video mask mode.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTxSs core instance.

Returns
  Current mode. 0 = Video masking is disabled 1 = Video masking is enabled

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

int XV_HdmiTxSs_IsStreamConnected | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function checks if the interface is connected.

Parameters

  None. |

Returns
  - TRUE if the interface is connected.
  - FALSE if the interface is not connected.

Note
  None.

References XV_HdmiTxSs::IsStreamConnected.

int XV_HdmiTxSs_IsStreamToggled | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function checks if the interface has toggled.

Parameters

  None. |

Returns
  - TRUE if the interface HPD has toggled.
  - FALSE if the interface HPD has not toggled.

Note
  None.

References XV_HdmiTxSs::IsStreamToggled.

int XV_HdmiTxSs_IsStreamUp | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function checks if the video stream is up.

Parameters

  None. |

Returns
  - TRUE if stream is up.
  - FALSE if stream is down.

Note
  None.

References XV_HdmiTxSs::IsStreamUp.

void XV_HdmiTxSS_MaskDisable | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function will disable the video masking.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTxSs core instance.

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

void XV_HdmiTxSS_MaskEnable | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function will enable the video masking.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTxSs core instance.

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

Referenced by XV_HdmiTxSS_SetBackgroundColor().

void XV_HdmiTxSS_MaskNoise | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | Enable
| ) |  |

This function will enable or disable the noise in the video mask.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTxSs core instance.
  Enable | specifies TRUE/FALSE value to either enable or disable the Noise.

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

Referenced by XV_HdmiTxSS_SetBackgroundColor().

void XV_HdmiTxSS_MaskSetBlue | ( | XV_HdmiTxSs * | InstancePtr,
|  | u16 | Value
| ) |  |

This function will set the blue component in the video mask.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTxSs core instance.
  Value | specifies the video mask value set to blue component

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

Referenced by XV_HdmiTxSS_SetBackgroundColor().

void XV_HdmiTxSS_MaskSetGreen | ( | XV_HdmiTxSs * | InstancePtr,
|  | u16 | Value
| ) |  |

This function will set the green component in the video mask.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTxSs core instance.
  Value | specifies the video mask value set to green component

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

Referenced by XV_HdmiTxSS_SetBackgroundColor().

void XV_HdmiTxSS_MaskSetRed | ( | XV_HdmiTxSs * | InstancePtr,
|  | u16 | Value
| ) |  |

This function will set the red component in the video mask.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTxSs core instance.
  Value | specifies the video mask value set to red component

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

Referenced by XV_HdmiTxSS_SetBackgroundColor().

int XV_HdmiTxSs_ReadEdid | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 * | Buffer
| ) |  |

This function reads the HDMI Sink EDID.

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr, and XV_HdmiTxSs::IsStreamConnected.

int XV_HdmiTxSs_ReadEdidSegment | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 * | Buffer,
|  | u8 | segment
| ) |  |

This function reads one block from the HDMI Sink EDID.

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr, and XV_HdmiTxSs::IsStreamConnected.

Referenced by XV_HdmiTxSs_ShowEdid().

void XV_HdmiTxSs_RefClockChangeInit | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function is called when HDMI TX SS TMDS clock changes.

Parameters

  None. |

Returns
  None

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr, XV_HdmiTxSs_SYSRST(), XV_HdmiTxSs_TXCore_LRST(), XV_HdmiTxSs_TXCore_VRST(), and XV_HdmiTxSs_VRST().

void XV_HdmiTxSs_ReportInfo | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function prints the HDMI TX SS subcore versions.

Parameters

  None. |

Returns
  None.

Note
  None.

void XV_HdmiTxSs_Reset | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function resets the video subsystem sub-cores.

There are 2 reset networks within the subsystem

- For cores that are on AXIS interface
- For cores that are on AXI-MM interface

Parameters

  InstancePtr | is a pointer to the Subsystem instance to be worked on.

Returns
  None

References XV_HDMITXSS_LOG_EVT_RESET, XV_HdmiTxSs_LogWrite(), XV_HdmiTxSs_SYSRST(), XV_HdmiTxSs_TXCore_LRST(), XV_HdmiTxSs_TXCore_VRST(), and XV_HdmiTxSs_VRST().

Referenced by XV_HdmiTxSs_CfgInitialize().

void XV_HdmiTxSs_SendAuxInfoframe | ( | XV_HdmiTxSs * | InstancePtr,
|  | void * | Aux
| ) |  |

This function sends audio info frames.

Parameters

  None. |

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

u32 XV_HdmiTxSs_SendGenericAuxInfoframe | ( | XV_HdmiTxSs * | InstancePtr,
|  | void * | Aux
| ) |  |

This function sends generic info frames.

Parameters

  None. |

Returns
  - XST_SUCCESS if infoframes transmitted successfully.
  - XST_FAILURE if AUX FIFO is full.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

void XV_HdmiTxSS_SetAppVersion | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | maj,
|  | u8 | min
| ) |  |

This function will set the major and minor application version in TXSs struct.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTxSs core instance.
  maj | is the major version of the application.
  min | is the minor version of the application.

Returns
  void.

Note
  None.

References XV_HdmiTxSs::AppMajVer, and XV_HdmiTxSs::AppMinVer.

void XV_HdmiTxSs_SetAudioChannels | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | AudioChannels
| ) |  |

This function Sets the HDMI TX SS number of active audio channels.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance
  AudioChannels |

Returns
  None.

Note
  None.

References XV_HdmiTxSs::AudioChannels, XV_HdmiTxSs::AudioInfoframe, XV_HdmiTxSs::HdmiTxPtr, XV_HDMITXSS_LOG_EVT_SETAUDIOCHANNELS, and XV_HdmiTxSs_LogWrite().

void XV_HdmiTxSs_SetAudioFormat | ( | XV_HdmiTxSs * | InstancePtr,
|  | XV_HdmiTx_AudioFormatType | format
| ) |  |

This function Sets the HDMI TX SS Audio Format.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance
  format | 1:HBR 0:L-PCM

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

void XV_HdmiTxSS_SetBackgroundColor | ( | XV_HdmiTxSs * | InstancePtr,
|  | XVMaskColorId | ColorId
| ) |  |

This function configures the background color for Video Masking Feature.

Parameters

  InstancePtr | is a pointer to the core instance to be worked on.
  ColorId | is the background color requested

Returns
  None

References XV_HdmiTxSs::HdmiTxPtr, XV_HdmiTxSs_GetVideoStream(), XV_HdmiTxSS_MaskEnable(), XV_HdmiTxSS_MaskNoise(), XV_HdmiTxSS_MaskSetBlue(), XV_HdmiTxSS_MaskSetGreen(), and XV_HdmiTxSS_MaskSetRed().

int XV_HdmiTxSs_SetCallback | ( | XV_HdmiTxSs * | InstancePtr,
|  | XV_HdmiTxSs_HandlerType | HandlerType,
|  | void * | CallbackFunc,
|  | void * | CallbackRef
| ) |  |

This function installs an asynchronous callback function for the given HandlerType:

    HandlerType                     Callback Function Type
    -----------------------         ---------------------------------------------
    (XV_HDMITXSS_HANDLER_CONNECT)       HpdCallback
    (XV_HDMITXSS_HANDLER_VS)            VsCallback
    (XV_HDMITXSS_HANDLER_STREAM_DOWN)   StreamDownCallback
    (XV_HDMITXSS_HANDLER_STREAM_UP)     StreamUpCallback
    (XV_HDMITXSS_HANDLER_BRDGOVERFLOW)  BrdgOverflowCallback
    (XV_HDMITXSS_HANDLER_BRDGUNDERFLOW) BrdgUnderflowCallback
    (XV_HDMITXSS_HANDLER_HDCP_AUTHENTICATED)
    (XV_HDMITXSS_HANDLER_HDCP_DOWNSTREAM_TOPOLOGY_AVAILABLE)
    (XV_HDMITXSS_HANDLER_HDCP_UNAUTHENTICATED)

Parameters

  InstancePtr | is a pointer to the HDMI TX Subsystem instance.
  HandlerType | specifies the type of handler.
  CallbackFunc | is the address of the callback function.
  CallbackRef | is a user data item that will be passed to the callback function when it is invoked.

Returns
  - XST_SUCCESS if callback function installed successfully.
  - XST_INVALID_PARAM when HandlerType is invalid.

Note
  Invoking this function for a handler that already has been installed replaces it with the new handler.

References XV_HdmiTxSs::BrdgOverflowCallback, XV_HdmiTxSs::BrdgOverflowRef, XV_HdmiTxSs::BrdgUnderflowCallback, XV_HdmiTxSs::BrdgUnderflowRef, XV_HdmiTxSs::BrdgUnlockedCallback, XV_HdmiTxSs::BrdgUnlockedRef, XV_HdmiTxSs::ConnectCallback, XV_HdmiTxSs::ConnectRef, XV_HdmiTxSs::StreamDownCallback, XV_HdmiTxSs::StreamDownRef, XV_HdmiTxSs::StreamUpCallback, XV_HdmiTxSs::StreamUpRef, XV_HdmiTxSs::ToggleCallback, XV_HdmiTxSs::ToggleRef, XV_HdmiTxSs::VsCallback, XV_HdmiTxSs::VsRef, XV_HDMITXSS_HANDLER_BRDGOVERFLOW, XV_HDMITXSS_HANDLER_BRDGUNDERFLOW, XV_HDMITXSS_HANDLER_BRDGUNLOCK, XV_HDMITXSS_HANDLER_CONNECT, XV_HDMITXSS_HANDLER_HDCP_AUTHENTICATED, XV_HDMITXSS_HANDLER_HDCP_DOWNSTREAM_TOPOLOGY_AVAILABLE, XV_HDMITXSS_HANDLER_HDCP_UNAUTHENTICATED, XV_HDMITXSS_HANDLER_STREAM_DOWN, XV_HDMITXSS_HANDLER_STREAM_UP, XV_HDMITXSS_HANDLER_TOGGLE, and XV_HDMITXSS_HANDLER_VS.

void XV_HdmiTxSs_SetDefaultPpc | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | Id
| ) |  |

This function will set the default in HDF.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTxSs core instance.
  Id | is the XV_HdmiTxSs ID to operate on.

Returns
  None.

Note
  None.

References XV_HdmiTxSs::Config, and XV_HdmiTxSs_Config::Ppc.

void XV_HdmiTxSS_SetDviMode | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function sets the core into DVI mode.

Parameters

  InstancePtr | is a pointer to the HDMI TX Subsystem

References XV_HdmiTxSs::HdmiTxPtr.

Referenced by XV_HdmiTxSs_SetVideoStreamType().

void XV_HdmiTxSs_SetGcpAvmuteBit | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function sets the HDMI TX AUX GCP register AVMUTE bit.

Parameters

  InstancePtr | is a pointer to the Subsystem instance to be worked on.

Returns
  None

References XV_HdmiTxSs::HdmiTxPtr.

void XV_HdmiTxSs_SetGcpClearAvmuteBit | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function sets the HDMI TX AUX GCP register CLEAR_AVMUTE bit.

Parameters

  InstancePtr | is a pointer to the Subsystem instance to be worked on.

Returns
  None

References XV_HdmiTxSs::HdmiTxPtr.

void XV_HdmiTxSS_SetHdmiMode | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function sets the core into HDMI mode.

Parameters

  InstancePtr | is a pointer to the HDMI TX Subsystem

References XV_HdmiTxSs::HdmiTxPtr.

Referenced by XV_HdmiTxSs_SetVideoStreamType(), and XV_HdmiTxSs_SubcoreInitHdmiTx().

void XV_HdmiTxSS_SetHpdTolerance | ( | XV_HdmiTxSs * | InstancePtr,
|  | XV_HdmiTxSs_HpdToleranceType | Type,
|  | u16 | ToleranceVal
| ) |  |

This function will Configure Timegrid based on the tolerance value for HPD and Toggle event.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTxSs core instance.
  Type | is the tolerance type.
  ToleranceVal | is the tolerance value to be applied.

Returns
  void.

Note
  None.

References XV_HdmiTxSs_Config::BaseAddress, and XV_HdmiTxSs::Config.

void XV_HdmiTxSs_SetPpc | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | Id,
|  | u8 | Ppc
| ) |  |

This function will set PPC specified by user.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTxSs core instance.
  Id | is the XV_HdmiTxSs ID to operate on.
  Ppc | is the PPC to be set.

Returns
  None.

Note
  None.

References XV_HdmiTxSs::Config, and XV_HdmiTxSs_Config::Ppc.

void XV_HdmiTxSs_SetSamplingRate | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | SamplingRate
| ) |  |

This function Sets the HDMI TX SS video Identification code.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance
  SamplingRate | Value

Returns
  None.

Note
  None.

References XV_HdmiTxSs::SamplingRate.

void XV_HdmiTxSs_SetScrambler | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | Enable
| ) |  |

This function enables / disables the TX scrambler.

Parameters

  InstancePtr | is a pointer to the Subsystem instance to be worked on.
  Enable | TRUE:Enable scrambler FALSE:Disable scrambler

Returns
  None.

Note
  The scrambler setting will revert to the default behavior during the next stream configuration (scrambler is enabled for HDMI 2.0 video and disabled when the video is of HDMI 1.4 or lower)

References XV_HdmiTxSs::HdmiTxPtr, and XV_HdmiTxSs_SetVideoStreamScramblingFlag().

u32 XV_HdmiTxSs_SetStream | ( | XV_HdmiTxSs * | InstancePtr,
|  | XVidC_VideoMode | VideoMode,
|  | XVidC_ColorFormat | ColorFormat,
|  | XVidC_ColorDepth | Bpc,
|  | XVidC_3DInfo * | Info3D
| ) |  |

This function set HDMI TX susbsystem stream parameters.

Parameters

  None. |

Returns
  Calculated TMDS Clock

Note
  None.

References XV_HdmiTxSs::Config, XV_HdmiTxSs::HdmiTxPtr, XV_HdmiTxSs_Config::Ppc, XV_HDMITXSS_LOG_EVT_SETSTREAM, and XV_HdmiTxSs_LogWrite().

void XV_HdmiTxSs_SetTmdsClockRatio | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | Ratio
| ) |  |

This function Sets the HDMI TX SS TMDS Cock Ratio.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance
  Ratio | 0 - 1/10, 1 - 1/40

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

void XV_HdmiTxSs_SetVideoIDCode | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | Vic
| ) |  |

This function Sets the HDMI TX SS video Identification code.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance
  InstancePtr | VIC Flag Value

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

void XV_HdmiTxSs_SetVideoStream | ( | XV_HdmiTxSs * | InstancePtr,
|  | XVidC_VideoStream | VidStream
| ) |  |

This function Sets the HDMI TX SS video stream.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance
  @return | XVidC_VideoStream pointer

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

void XV_HdmiTxSs_SetVideoStreamScramblingFlag | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | IsScrambled
| ) |  |

This function Sets the HDMI TX SS video stream type.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance
  IsScrambled | 1:IsScrambled 0: not Scrambled

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

Referenced by XV_HdmiTxSs_SetScrambler().

void XV_HdmiTxSs_SetVideoStreamScramblingOverrideFlag | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | OverrideScramble
| ) |  |

This function Sets the HDMI TX SS video stream scrambling behaviour.

Setting OverrideScramble to true will force enabling/disabling scrambling function based on the value of IsScrambled flag.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance
  OverrideScramble | 0: Scrambling is always enabled for HDMI 2.0 resolutions and is enabled /or disabled for HDMI 1.4 resolutions based on IsScrambled value 1: Enable scrambling if IsScrambled is TRUE and disable scrambling if IsScrambled is FALSE

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr.

void XV_HdmiTxSs_SetVideoStreamType | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | StreamType
| ) |  |

This function Sets the HDMI TX SS video stream type.

Parameters

  InstancePtr | pointer to XV_HdmiTxSs instance
  InstancePtr | VIC Value 1:HDMI 0:DVI

Returns
  None.

Note
  None.

References XV_HdmiTxSs_AudioMute(), XV_HdmiTxSS_SetDviMode(), and XV_HdmiTxSS_SetHdmiMode().

void XV_HdmiTxSs_ShowEdid | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function shows the HDMI source edid.

Returns
  None.

Note
  None.

References XV_HdmiTxSs::IsStreamConnected, and XV_HdmiTxSs_ReadEdidSegment().

void XV_HdmiTxSs_Start | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function starts the HDMI TX subsystem including all sub-cores that are included in the processing pipeline for a given use-case.

Video pipe is started from back to front

Parameters

  InstancePtr | is a pointer to the Subsystem instance to be worked on.

Returns
  None

Note
  Cores are started only if the corresponding start flag in the scratch pad memory is set. This allows to selectively start only those cores included in the processing chain

References XV_HDMITXSS_LOG_EVT_START, and XV_HdmiTxSs_LogWrite().

void XV_HdmiTxSs_Stop | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function stops the HDMI TX subsystem including all sub-cores Stop the video pipe starting from front to back.

Parameters

  InstancePtr | is a pointer to the Subsystem instance to be worked on.

Returns
  None

References XV_HdmiTxSs::VtcPtr, XV_HDMITXSS_LOG_EVT_STOP, and XV_HdmiTxSs_LogWrite().

void XV_HdmiTxSs_StreamStart | ( | XV_HdmiTxSs * | InstancePtr | ) |

This function starts the HDMI TX stream.

Returns
  None.

Note
  None.

References XV_HdmiTxSs::HdmiTxPtr, XV_HDMITXSS_LOG_EVT_STREAMSTART, and XV_HdmiTxSs_LogWrite().

void XV_HdmiTxSs_SYSRST | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | Reset
| ) |  |

This function asserts or releases the system reset of other blocks within the subsystem.

Parameters

  InstancePtr | is a pointer to the Subsystem instance to be worked on.

Returns
  None

References XV_HdmiTxSs::HdmiTxPtr.

Referenced by XV_HdmiTxSs_RefClockChangeInit(), and XV_HdmiTxSs_Reset().

void XV_HdmiTxSs_TXCore_LRST | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | Reset
| ) |  |

This function asserts or releases the Internal Link reset of the HDMI subcore within the subsystem.

Parameters

  InstancePtr | is a pointer to the Subsystem instance to be worked on.

Returns
  None

References XV_HdmiTxSs::HdmiTxPtr.

Referenced by XV_HdmiTxSs_RefClockChangeInit(), and XV_HdmiTxSs_Reset().

void XV_HdmiTxSs_TXCore_VRST | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | Reset
| ) |  |

This function asserts or releases the Internal Video reset of the HDMI subcore within the subsystem.

Parameters

  InstancePtr | is a pointer to the Subsystem instance to be worked on.

Returns
  None

References XV_HdmiTxSs::HdmiTxPtr.

Referenced by XV_HdmiTxSs_RefClockChangeInit(), and XV_HdmiTxSs_Reset().

void XV_HdmiTxSs_VRST | ( | XV_HdmiTxSs * | InstancePtr,
|  | u8 | Reset
| ) |  |

This function asserts or releases the video reset of other blocks within the subsystem.

Parameters

  InstancePtr | is a pointer to the Subsystem instance to be worked on.

Returns
  None

References XV_HdmiTxSs::HdmiTxPtr.

Referenced by XV_HdmiTxSs_RefClockChangeInit(), and XV_HdmiTxSs_Reset().

## Variable Documentation

XV_HdmiTxSs_SubCores XV_HdmiTxSs_SubCoreRepo[XPAR_XV_HDMITXSS_NUM_INSTANCES]

Define Driver instance of all sub-core included in the design.