| dfemix Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfeMix_DUCDDCStatus Struct Reference
Overview

DUC/DDC status. More...

## Data Fields
u32 | Stage
| [0-3] Earliest stage in which overflow occurred. More...
u32 | Antenna
          [0-7] Antenna on which overflow occured, with lowest
antenna taking priority. More...
u32 | NcoId
        [0-15] Number of NCO associated with overflowing channel,
with lowest taking priority. More...

## Detailed Description

DUC/DDC status.

## Field Documentation

u32 XDfeMix_DUCDDCStatus::Antenna

          [0-7] Antenna on which overflow occured, with lowest

antenna taking priority.

Referenced by XDfeMix_GetDUCDDCStatus().

u32 XDfeMix_DUCDDCStatus::NcoId

        [0-15] Number of NCO associated with overflowing channel,

with lowest taking priority.

Referenced by XDfeMix_GetDUCDDCStatus().

u32 XDfeMix_DUCDDCStatus::Stage

[0-3] Earliest stage in which overflow occurred.

Referenced by XDfeMix_GetDUCDDCStatus().