| sdps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xsdps.c File Reference

## Functions
s32 | XSdPs_CfgInitialize (XSdPs *InstancePtr, XSdPs_Config *ConfigPtr, UINTPTR EffectiveAddr)
| Initializes a specific XSdPs instance so that the driver is ready to use. More...
s32 | XSdPs_CardInitialize (XSdPs *InstancePtr)
| Initializes Card with Identification mode sequence. More...
s32 | XSdPs_ReadPolled (XSdPs *InstancePtr, u32 Arg, u32 BlkCnt, u8 *Buff)
| Performs SD read in polled mode. More...
s32 | XSdPs_WritePolled (XSdPs *InstancePtr, u32 Arg, u32 BlkCnt, const u8 *Buff)
| Performs SD write in polled mode. More...
s32 | XSdPs_Idle (XSdPs *InstancePtr)
| API to idle the SDIO Interface. More...
s32 | XSdPs_Erase (XSdPs *InstancePtr, u32 StartAddr, u32 EndAddr)
| Performs Erase operation on the given address range. More...
s32 | XSdPs_Sanitize (XSdPs *InstancePtr)
| Performs Sanitize operation on the unmapped user address range. More...