| scugic Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XScuGic Struct Reference
SCUGIC APIs

The XScuGic driver instance data. More...

## Data Fields
XScuGic_Config * | Config
| Configuration table entry. More...
u32 | IsReady
| Device is initialized and ready. More...
u32 | UnhandledInterrupts
| Intc Statistics. More...

## Detailed Description

The XScuGic driver instance data.

The user is required to allocate a variable of this type for every intc device in the system. A pointer to a variable of this type is then passed to the driver API functions.