| hdcp22_tx Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XHdcp22_Tx_LogItem Struct Reference
Overview

This typedef is used to store logging events. More...

## Data Fields
u8 | LogEvent
| Event that has been triggered. More...
u16 | Data
| Optional data. More...
u32 | TimeStamp
| Time stamp on when event occurred. More...

## Detailed Description

This typedef is used to store logging events.

## Field Documentation

u16 XHdcp22_Tx_LogItem::Data

Optional data.

Referenced by XHdcp22Tx_LogDisplay(), XHdcp22Tx_LogRd(), and XHdcp22Tx_LogWr().

u8 XHdcp22_Tx_LogItem::LogEvent

Event that has been triggered.

Referenced by XHdcp22Tx_LogDisplay(), XHdcp22Tx_LogRd(), and XHdcp22Tx_LogWr().

u32 XHdcp22_Tx_LogItem::TimeStamp

Time stamp on when event occurred.

Only used for time critical events.

Referenced by XHdcp22Tx_LogDisplay(), XHdcp22Tx_LogRd(), and XHdcp22Tx_LogWr().