| nandps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions | Variables
xnandps_onfi.c File Reference

## Functions
void | XNandPs_SendCommand (XNandPs *InstancePtr, XNandPs_CommandFormat *Command, int Page, int Column)
| This function sends a NAND command to the flash device. More...
u8 | Onfi_CmdReadStatus (XNandPs *InstancePtr)
| This function sends read status command to the flash device. More...
int | Onfi_NandInit (XNandPs *InstancePtr)
| This function initializes the NAND flash and gets the geometry information. More...

## Variables
XNandPs_CommandFormat | OnfiCommands []
| This structure defines the onfi command format sent to the flash. More...