| hdcp22_tx_dp Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XHdcp22_Tx_Dp_PairingInfo Struct Reference
Overview

This typedef contains the the used keys used for authentication with stored Km. More...

## Data Fields
u8 | ReceiverId [5]
| Unique receiver Id. More...
u8 | RxCaps [3]
| Capabilities of the receiver. More...
u8 | Rtx [8]
| Random nonce for tx. More...
u8 | Rrx [8]
| Random nonce for Rx (m: Rtx || Rrx). More...
u8 | Km [16]
| Km. More...
u8 | Ekh_Km [16]
| Ekh(Km). More...
u8 | Ready
| Indicates a valid entry. More...

## Detailed Description

This typedef contains the the used keys used for authentication with stored Km.

## Field Documentation

u8 XHdcp22_Tx_Dp_PairingInfo::Ekh_Km[16]

Ekh(Km).

u8 XHdcp22_Tx_Dp_PairingInfo::Km[16]

Km.

u8 XHdcp22_Tx_Dp_PairingInfo::Ready

Indicates a valid entry.

u8 XHdcp22_Tx_Dp_PairingInfo::ReceiverId[5]

Unique receiver Id.

u8 XHdcp22_Tx_Dp_PairingInfo::Rrx[8]

Random nonce for Rx (m: Rtx || Rrx).

u8 XHdcp22_Tx_Dp_PairingInfo::Rtx[8]

Random nonce for tx.

u8 XHdcp22_Tx_Dp_PairingInfo::RxCaps[3]

Capabilities of the receiver.