| dfemix Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfeMix_AuxiliaryCfg Struct Reference
Overview

Defines settings for single auxiliary NCO. More...

## Data Fields
u32 | Enable
| [0,1] Auxiliary NCO Enable: More...
u32 | AuxGain
| [0-3] Auxiliary NCO gain. More...

## Detailed Description

Defines settings for single auxiliary NCO.

## Field Documentation

u32 XDfeMix_AuxiliaryCfg::AuxGain

[0-3] Auxiliary NCO gain.

- 0 = MINUS18DB: Apply -18dB gain.
- 1 = MINUS12DB: Apply -12dB gain.
- 2 = MINUS6DB: Apply -6dB gain.
- 3 = ZERODB: Apply -0dB gain.

u32 XDfeMix_AuxiliaryCfg::Enable

[0,1] Auxiliary NCO Enable:

- 0 = disabled
- 1 = enabled

Referenced by XDfeMix_RemoveAuxNCOfromCCCfg().