| intc Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xintc_l.c File Reference

## Functions
XIntc_Config * | LookupConfigByBaseAddress (UINTPTR BaseAddress)
| Looks up the device configuration based on the base address of the device. More...
void | XIntc_DeviceInterruptHandler (void *DeviceId)
| This function is the primary interrupt handler for the driver. More...
void | XIntc_SetIntrSvcOption (UINTPTR BaseAddress, int Option)
| Set the interrupt service option, which can configure the driver so that it services only a single interrupt at a time when an interrupt occurs, or services all pending interrupts when an interrupt occurs. More...
void | XIntc_RegisterHandler (UINTPTR BaseAddress, int InterruptId, XInterruptHandler Handler, void *CallBackRef)
| Register a handler function for a specific interrupt ID. More...
void | XIntc_RegisterFastHandler (UINTPTR BaseAddress, u8 Id, XFastInterruptHandler FastHandler)
| Register a fast handler function for a specific interrupt ID. More...