| v_hdmirxss1 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xv_hdmirxss1_frl.c File Reference

## Overview

This is main code of Xilinx HDMI Transmitter Subsystem device driver.

Please see xv_hdmirxss1.h for more details of the driver.

    MODIFICATION HISTORY:

    Ver   Who    Date     Changes

    1.00  EB   22/05/18 Initial release.

## Functions
void | XV_HdmiRxSs1_FrlConfigCallback (void *CallbackRef)
| This function is called when the FRL link training requires configuration from application. More...
void | XV_HdmiRxSs1_FrlStartCallback (void *CallbackRef)
| This function is called when the FRL link training passes and sink is ready to receive video, audio and control packets. More...
void | XV_HdmiRxSs1_TmdsConfigCallback (void *CallbackRef)
| This function is called when during FRL link training, it is decided to fallback to the legacy HDMI TMDS mode. More...

## Function Documentation

void XV_HdmiRxSs1_FrlConfigCallback | ( | void * | CallbackRef | ) |

This function is called when the FRL link training requires configuration from application.

Parameters

  None. |

Returns
  None.

Note
  None.

References XV_HdmiRxSs1::FrlConfigCallback, and XV_HdmiRxSs1::FrlConfigRef.

void XV_HdmiRxSs1_FrlStartCallback | ( | void * | CallbackRef | ) |

This function is called when the FRL link training passes and sink is ready to receive video, audio and control packets.

Parameters

  None. |

Returns
  None.

Note
  None.

References XV_HdmiRxSs1::FrlStartCallback, XV_HdmiRxSs1::FrlStartRef, and XV_HdmiRxSs1_LogWrite().

void XV_HdmiRxSs1_TmdsConfigCallback | ( | void * | CallbackRef | ) |

This function is called when during FRL link training, it is decided to fallback to the legacy HDMI TMDS mode.

Parameters

  None. |

Returns
  None.

Note
  None.

References XV_HdmiRxSs1::TmdsConfigCallback, and XV_HdmiRxSs1::TmdsConfigRef.