| v_hdmitx1 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XV_HdmiTx1_Config Struct Reference

This typedef contains configuration information for the HDMI TX core. More...

## Data Fields
u16 | DeviceId
| DeviceId is the unique ID of the HDMI TX core. More...
UINTPTR | BaseAddress
| BaseAddress is the physical base address of the core's registers. More...
u32 | MaxFrlRate
| Maximum FRL Rate Supported. More...
u32 | DynHdr
| Dynamic HDR supported. More...

## Detailed Description

This typedef contains configuration information for the HDMI TX core.

Each HDMI TX device should have a configuration structure associated.

## Field Documentation

UINTPTR XV_HdmiTx1_Config::BaseAddress

BaseAddress is the physical base address of the core's registers.

Referenced by XV_HdmiTx1_Aux_Dsc_Send_Data(), XV_HdmiTx1_Aux_Dsc_Send_Header(), XV_HdmiTx1_AuxSend(), XV_HdmiTx1_CfgInitialize(), XV_HdmiTx1_DdcGetAck(), XV_HdmiTx1_DdcInit(), XV_HdmiTx1_DdcReadData(), XV_HdmiTx1_DdcWaitForDone(), XV_HdmiTx1_DdcWriteCommand(), XV_HdmiTx1_DebugInfo(), XV_HdmiTx1_IntrHandler(), XV_HdmiTx1_RegisterDebug(), XV_HdmiTx1_SelfTest(), XV_HdmiTx1_SetColorDepth(), XV_HdmiTx1_SetColorFormat(), XV_HdmiTx1_SetPixelRate(), and XV_HdmiTx1_SetSampleRate().

u16 XV_HdmiTx1_Config::DeviceId

DeviceId is the unique ID of the HDMI TX core.

u32 XV_HdmiTx1_Config::DynHdr

Dynamic HDR supported.

u32 XV_HdmiTx1_Config::MaxFrlRate

Maximum FRL Rate Supported.

Referenced by XV_HdmiTx1_CfgInitialize(), and XV_HdmiTx1_SetFrlMaxFrlRate().