| emacps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xemacps_pcs.c File Reference

## Functions
void | XEmacPs_SetupPCS (XEmacPs *EmacPsInstancePtr)
| Set up PCS as follows for every given speed: More...
bool | XEmacPs_USXPCSGetState (UINTPTR BaseAddr)
| Get USX synchronisation status. More...
bool | XEmacPs_IsHighSpeedPCS (UINTPTR BaseAddr)
| Detect if the device supports High Speeds ( 5G, 10G ) More...