| axidma Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xaxidma_example_selftest.c File Reference

## Overview

This file demonstrates the example to do selftest on the device.

    MODIFICATION HISTORY:

    Ver   Who  Date     Changes
    ----- ---- -------- -------------------------------------------------------
    9.3   ms   01/23/17 Modified xil_printf statement in main function to
                        ensure that "Successfully ran" and "Failed" strings are
                        available in all examples. This is a fix for CR-965028.
          ms   04/05/17 Modified Comment lines in functions to
                        recognize it as documentation block for doxygen
                        generation of examples.

## Functions
int | AxiDMASelfTestExample (u16 DeviceId)
| This function performance a reset of the DMA device and checks the device is coming out of reset or not. More...
int | main ()
| The entry point for this example. More...

## Function Documentation

int AxiDMASelfTestExample | ( | u16 | DeviceId | ) |

This function performance a reset of the DMA device and checks the device is coming out of reset or not.

Parameters

  DeviceId | is the DMA device id.

Returns
  - XST_SUCCESS if channel reset is successful
  - XST_FAILURE if channel reset fails.

Note
  None.

References XAxiDma_CfgInitialize(), XAxiDma_LookupConfig(), and XAxiDma_Selftest().

Referenced by main().

int main | ( | void |  | ) |

The entry point for this example.

It invokes the example function, and reports the execution status.

Parameters

  None. |

Returns
  - XST_SUCCESS if example finishes successfully
  - XST_FAILURE if example fails.

Note
  None.

References AxiDMASelfTestExample().