| tmrctr Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xtmrctr_selftest_example.c File Reference

## Overview

This file contains a example for using the Timer Counter hardware and driver.

Note

None

    MODIFICATION HISTORY:

    Ver   Who  Date  Changes

    1.00a sv   04/25/05 Initial release for TestApp integration.
    2.00a ktn  11/26/09 Minor changes as per coding guidelines.
    4.2   ms   01/23/17 Added xil_printf statement in main function to
                        ensure that "Successfully ran" and "Failed" strings
                        are available in all examples. This is a fix for
                        CR-965028.

## Functions
int | TmrCtrSelfTestExample (u16 DeviceId)
| This function does a minimal test on the TmrCtr device and driver as a design example. More...
int | main (void)
| Main function to call the example. More...

## Function Documentation

int main | ( | void |  | ) |

Main function to call the example.

This function is not included if the example is generated from the TestAppGen test tool.

Parameters

  None |

Returns
  XST_SUCCESS to indicate success, else XST_FAILURE to indicate a Failure.

Note
  None

References TmrCtrSelfTestExample().

int TmrCtrSelfTestExample | ( | u16 | DeviceId | ) |

This function does a minimal test on the TmrCtr device and driver as a design example.

The purpose of this function is to illustrate how to use the XTmrCtr component.

Parameters

  DeviceId | is the XPAR_<TMRCTR_instance>_DEVICE_ID value from xparameters.h
  TmrCtrNumber | is the timer counter of the device to operate on. Each device may contain multiple timer counters. The timer number is a zero based number with a range of 0 - (XTC_DEVICE_TIMER_COUNT - 1).

Returns
  XST_SUCCESS if successful, XST_FAILURE if unsuccessful

Note
  None

References XTmrCtr_Initialize(), and XTmrCtr_SelfTest().

Referenced by main().