| axiethernet Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XAvb_Config Struct Reference

This typedef contains configuration information for a device. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
u32 | BaseAddress
| Register base address. More...

## Detailed Description

This typedef contains configuration information for a device.

## Field Documentation

u32 XAvb_Config::BaseAddress

Register base address.

Referenced by main(), XAvb_BecomeRtcMaster(), XAvb_CalcRtcOffset(), XAvb_CfgInitialize(), XAvb_DecodeRxAnnounceFrame(), XAvb_DecodeRxFollowUp(), XAvb_DecodeRxPDelayResp(), XAvb_DecodeRxPDelayRespFollowUp(), XAvb_DecodeRxSignaling(), XAvb_DecodeRxSync(), XAvb_DecodeTxAnnounceFrame(), XAvb_IsRxFramePTP(), XAvb_MasterSendAnnounce(), XAvb_MasterSendFollowUp(), XAvb_MasterSendSync(), XAvb_PtpRxInterruptHandler(), XAvb_PtpTimerInterruptHandler(), XAvb_Reset(), XAvb_SendPDelayReq(), XAvb_SendPDelayResp(), XAvb_SendPDelayRespFollowUp(), XAvb_SetupRxFilterControlMatchMode(), XAvb_SetupRxFilterControlPcp(), XAvb_SetupRxFilterControlVid(), XAvb_SetupSourcePortIdentity(), XAvb_UpdateRtcIncrement(), and XAvb_WaitOnTxPtpQueue().

u16 XAvb_Config::DeviceId

Unique ID of device.

Referenced by main().