| mipicsiss Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Data Structures | Enumerations | Functions
ti_tmds1204.h File Reference

## Data Structures
struct | Ti_RegisterField
| This typedef contains translations of FRL_Rate to Lanes and Line Rates. More...

## Enumerations
enum | Ti_DeviceType
| FRL Character Rate Enumeration. More...

## Functions
int | TI_TMDS1204_Init (void *IicPtr, u8 I2CSlaveAddress, u8 Revision, u8 IsTx)
| This function initializes the TI TMDS1204 with default values for use with the Video FMC. More...
int | TI_TMDS1204_CheckDeviceID (void *IicPtr, u8 I2CSlaveAddress)
| This function checks the TI TMDS1204 device ID. More...
u8 | TI_TMDS1204_CheckDeviceVersion (void *IicPtr, u8 I2CSlaveAddress)
| This function checks the TI TMDS1204 Device Revision Number. More...
int | TI_TMDS1204_LineRateReconfig (void *IicPtr, u8 I2CSlaveAddress, u8 Revision, u8 IsFRL, u64 LineRate, u8 Lanes, u8 IsTx)
| This function reconfigures the TI TMDS1204 cable redriver. More...
void | TI_TMDS1204_RegisterDump (void *IicPtr, u8 I2CSlaveAddress)
| This function displays a registerdump of the TI TMDS1204 device. More...
void | TI_TMDS1204_RegisterLibraryDump (void)
| This function prints out all the contents from TiRegisterFields array. More...