| v_hcresampler Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

xv_hcresampler_l2.c File Reference

## Functions
Hw Configuration
The following constants define the horiz. resampler HW MAX configuration
int | XV_HcrsmplInitialize (XV_Hcresampler_l2 *InstancePtr, u16 DeviceId)
| This function initializes the core instance. More...
void | XV_HCrsmplStart (XV_Hcresampler_l2 *InstancePtr)
| This function starts the Chroma resampler core. More...
void | XV_HCrsmplStop (XV_Hcresampler_l2 *InstancePtr)
| This function stops the Chroma resampler core. More...
void | XV_HCrsmplLoadDefaultCoeff (XV_Hcresampler_l2 *InstancePtr)
| This function loads default filter coefficients in the chroma resampler coefficient storage based on the selected TAP configuration. More...
void | XV_HCrsmplrLoadExtCoeff (XV_Hcresampler_l2 *InstancePtr, u16 num_taps, const short *Coeff)
| This function loads user defined filter coefficients in the horiz. More...
void | XV_HCrsmplSetActiveSize (XV_Hcresampler_l2 *InstancePtr, u32 width, u32 height)
| This function configures the Chroma resampler active resolution. More...
void | XV_HCrsmplSetFormat (XV_Hcresampler_l2 *InstancePtr, XVidC_ColorFormat formatIn, XVidC_ColorFormat formatOut)
| This function configures the Chroma resampler for the required format conversion. More...
void | XV_HCrsmplDbgReportStatus (XV_Hcresampler_l2 *InstancePtr)
| This function prints Chroma Resampler status on the console. More...