| v_hdmitxss1 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
si570drv.c File Reference

## Overview

This file contains low-level driver functions for controlling the SiliconLabs Si570 clock generator as mounted on the ZCU106 demo board.

The user should refer to the hardware device specification for more details of the device operation.

    MODIFICATION HISTORY:

    Ver   Who Date         Changes

    1.0   ssh 07/28/2021      Initial release.

## Functions
void | Si570_SetFreq (void *IicPtr, u8 Si_Addr, double Freq)
| This function the frequency output of Si570. More...

## Function Documentation

void Si570_SetFreq | ( | void * | IicPtr,
|  | u8 | Si_Addr,
|  | double | Freq
| ) |  |

This function the frequency output of Si570.

Parameters

  IicPtr | IIC instance pointer.
  Si_Addr | contains the 7 bit IIC address of the device to send the specified data to.
  Freq | is the requested frequency output in MHz (floating)

Returns
  None.

Note
  None.

Referenced by Exdes_SetupClkSrc().