| clk_wiz Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Examples

You can refer to the below stated example applications for more details on how to use clk_wiz driver.

# xclk_wiz_intr_example.c

Contains an example on how to use the XClk_wiz driver directly. This example uses the XClk_Wiz driver with interrupts. It will generate interrupt for clok glitch, clock overflow and underflow. The user should have setup with 2 clocking wizard instances, one instance act as clocking monitor (Enable clock monitor in GUI), In another instance enable dynamic clock reconfiguration.

For details, see xclk_wiz_intr_example.c.