| resetps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

resetps Documentation

The Xilinx Reset Controller driver supports the following features:

- Assert reset for specific peripheral.
- Deassert reset for specific peripheral.
- Pulse reset for specific peripheral.
- Get reset status for specific peripheral.

This driver is intended to be RTOS and processor independent. It works with physical addresses only. Any needs for dynamic memory management, threads or thread mutual exclusion, virtual memory, or cache control must be satisfied by the layer above this driver.

    MODIFICATION HISTORY:
    Ver   Who    Date     Changes

    1.00  cjp    09/05/17 First release
    1.1   Nava   04/20/18 Fixed compilation warnings.
    1.2   cjp    04/27/18 Updated for clockps interdependency
    1.2   sd     07/20/18 Fixed Doxygen Reported warnings.
    1.4   sk     09/01/20 Updated the Makefile to support parallel make
                          execution.
    1.5   sk     11/30/21 Fix compilation warnings reported with "-Wundef" flag.
    1.6   sd     07/07/23 Added SDT support.
    1.7   sd     11/07/23 Remove the unused pss ref frequency