| scuwdt Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XScuWdt Struct Reference
Overview

The XScuWdt driver instance data. More...

## Data Fields
XScuWdt_Config | Config
| Hardware Configuration. More...
u32 | IsReady
| Device is initialized and ready. More...
u32 | IsStarted
| Device watchdog timer is running. More...

## Detailed Description

The XScuWdt driver instance data.

The user is required to allocate a variable of this type for every watchdog/timer device in the system. A pointer to a variable of this type is then passed to the driver API functions.

## Field Documentation

XScuWdt_Config XScuWdt::Config

Hardware Configuration.

Referenced by ScuWdtIntrExample(), XScuWdt_CfgInitialize(), XScuWdt_Start(), and XScuWdt_Stop().

u32 XScuWdt::IsReady

Device is initialized and ready.

Referenced by XScuWdt_CfgInitialize(), XScuWdt_SelfTest(), XScuWdt_Start(), and XScuWdt_Stop().

u32 XScuWdt::IsStarted

Device watchdog timer is running.

Referenced by XScuWdt_CfgInitialize(), XScuWdt_Start(), and XScuWdt_Stop().