| uartns550 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XUartNs550Format Struct Reference
Overview

This data type allows the data format of the device to be set and retrieved. More...

## Data Fields
u32 | BaudRate
| In bps, ie 1200. More...
u32 | DataBits
| Number of data bits. More...
u32 | Parity
| Parity. More...
u8 | StopBits
| Number of stop bits. More...

## Detailed Description

This data type allows the data format of the device to be set and retrieved.

## Field Documentation

u32 XUartNs550Format::BaudRate

In bps, ie 1200.

Referenced by XUartNs550_GetDataFormat(), and XUartNs550_SetDataFormat().

u32 XUartNs550Format::DataBits

Number of data bits.

Referenced by XUartNs550_GetDataFormat(), and XUartNs550_SetDataFormat().

u32 XUartNs550Format::Parity

Parity.

Referenced by XUartNs550_GetDataFormat(), and XUartNs550_SetDataFormat().

u8 XUartNs550Format::StopBits

Number of stop bits.

Referenced by XUartNs550_GetDataFormat(), and XUartNs550_SetDataFormat().