| v_hdmitx Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

Data Structures | Macros
xv_hdmitx.h File Reference

## Overview

This is the main header file for Xilinx HDMI TX core.

HDMI TX core is used for transmitting the incoming video and audio streams. It consists of

- Transmitter core
- AXI4-Stream to Video Bridge
- Video Timing Controller and
- High-bandwidth Digital Content Protection (HDCP) (Optional).

The HDMI TX uses three AXI interfaces for Video, Audio and Processor:

- AXI4-Stream interface for Video, can be single, dual or quad pixels per clock and supports 8 and 10 bits per component.
- AXI4-Stream interface for Audio, accepts multiple channels uncompressed and compressed audio data.
- AXI4-Lite interface for processor, controls the transmitter. Please do refer AXI Reference Guide (UG761) for more information on AXI interfaces.

Transmitter core performs following operations:

- Converts video data from the video clock domain into the link clock domain.
- TMDS (Transition Minimized Differential Signaling) encoding.
- Merges encoded video data and packet data into a single HDMI stream.
- Optional HDMI stream is encrypted by an external HDCP module.
- Over samples HDMI stream if stream bandwidth is too low for the transceiver to handle.
- Scrambles encrypted/HDMI stream if data rate is above 3.4 Gbps otherwise bypasses the Scrambler.

AXI Video Bridge converts the incoming video AXI-stream to native video.

Video Timing Controller (VTC) generates the native video timing.

Core Features

For a full description of HDMI TX features, please see the hardware specification.

Software Initialization & Configuration

The application needs to do following steps in order for preparing the HDMI TX core to be ready.

- Call XV_HdmiTx_LookupConfig using a device ID to find the core configuration.
- Call XV_HdmiTx_CfgInitialize to initialize the device and the driver instance associated with it.

Interrupts

This driver provides interrupt handlers

- XV_HdmiTx_IntrHandler, for handling the interrupts from the HDMI TX core PIO and DDC peripheral respectively.

Application developer needs to register interrupt handler with the processor, within their examples. Whenever processor calls registered application's interrupt handler associated with interrupt id, application's interrupt handler needs to call appropriate peripheral interrupt handler reading peripheral's Status register.

This driver provides XV_HdmiTx_SetCallback API to register functions with HDMI TX core instance.

Virtual Memory

This driver supports Virtual Memory. The RTOS is responsible for calculating the correct device base address in Virtual Memory space.

Threads

This driver is not thread safe. Any needs for threads or thread mutual exclusion must be satisfied by the layer above this driver.

Asserts

Asserts are used within all Xilinx drivers to enforce constraints on argument values. Asserts can be turned off on a system-wide basis by defining at compile time, the NDEBUG identifier. By default, asserts are turned on and it is recommended that users leave asserts on during development.

Building the driver

The HDMI TX driver is composed of several source files. This allows the user to build and link only those parts of the driver that are necessary.

     MODIFICATION HISTORY:
    s
     Ver   Who    Date     Changes

     1.00         10/07/15 Initial release.
     1.1   yh     15/01/16 Add 3D Support
     1.2   MG     09/03/16 Added XV_HdmiTx_SetHdmiMode and XV_HdmiTx_SetDviMode.
                           Removed support for reduced blanking
     1.3   YH     25/07/16 Used UINTPTR instead of u32 for BaseAddress
                           XV_HdmiTx_Config
                           XV_HdmiTx_CfgInitialize
     1.4   YH     17/08/16 Added XV_HdmiTx_SetAxiClkFreq
     1.5   YH     14/11/16 Added XV_HdmiTx_Bridge_yuv420 & XV_HdmiTx_Bridge_pixel
                           mode macros
     1.6   MG     28/03/17 Added XV_HdmiTx_Mask macros
     1.7   YH     19/07/17 Added XV_HdmiTx_IsMasked macro
                  22/08/17 Added XV_HdmiTx_Audio_LPCM macro
                           Added XV_HdmiTx_Audio_HBR macro
     1.8   YH     06/10/17 Replaced XV_HdmiTx_Audio_LPCM and XV_HdmiTx_Audio_HBR
                               macro with API XV_HdmiTx_SetAudioFormat
                           Added XV_HdmiTx_GetAudioFormat
     1.9   EB     24/10/17 Added enum XV_HdmiTx_AudioFormatType
     1.10  MMO    19/12/17 Added XV_HdmiTx_SetTmdsClk API
     2.0   EB     16/01/18 Updated function XV_HdmiTx_SetTmdsClk and renamed to
                               XV_HdmiTx_ConfigTmdsClk
                           Moved Vendor Specific InfoFrame related functions to
                               HDMI Common library
                           Deprecating XV_HdmiTx_VSIF_GeneratePacket,
                               XV_HdmiTx_VSIF_DisplayInfo,
                               XV_HdmiTx_VSIF_3DStructToString,
                               XV_HdmiTx_VSIF_3DSampMethodToString and
                               XV_HdmiTx_VSIF_3DSampPosToString APIs
                           Moved VicTable, XV_HdmiTx_Aux to Hdmi Common library
           EB     24/01/18 Added OverrideHdmi14Scrambler to XV_HdmiTx_Stream
     2.2   EB     03/08/18 Marked XV_HdmiTx_AudioMute and XV_HdmiTx_AudioUnmute
                               as deprecated
           MMO    11/08/18 Added Bridge Overflow and Bridge Underflow (PIO IN)
     2.5   EB     02/12/18 Added 3D Audio Support

## Data Structures
struct | XV_HdmiTx_Config
| This typedef contains configuration information for the HDMI TX core. More...
struct | XV_HdmiTx_AudioStream
| This typedef contains audio stream specific data structure. More...
struct | XV_HdmiTx_Stream
| This typedef contains HDMI TX stream specific data structure. More...
struct | XV_HdmiTx
| The XV_HdmiTx driver instance data. More...

## Macros
#define | XV_HDMITX_H_
| Prevent circular inclusions by using protection macros. More...

## Enumerations
Handler Types
enum | XV_HdmiTx_HandlerType
| These constants specify different types of handler and used to differentiate interrupt requests from peripheral. More...
HDMI TX stream status
enum | XV_HdmiTx_State

## HDMI TX audio format
#define | XV_HdmiTx_GetTime1Ms(InstancePtr) (InstancePtr)->Config.AxiLiteClkFreq/1000
| This macro returns the clock cycles required to count up to 1MS with respect to AXI Lite Frequency. More...
#define | XV_HdmiTx_GetVersion(InstancePtr)
| This macro reads the TX version. More...
#define | XV_HdmiTx_Reset(InstancePtr, Reset)
| This macro asserts or releases the HDMI TX reset. More...
#define | XV_HdmiTx_SetScrambler(InstancePtr, SetClr)
| This macro controls the HDMI TX Scrambler. More...
#define | XV_HdmiTx_Bridge_yuv420(InstancePtr, SetClr)
| This macro controls the YUV420 mode for video bridge. More...
#define | XV_HdmiTx_Bridge_pixel(InstancePtr, SetClr)
| This macro controls the Pixel Repeat mode for video bridge. More...
#define | XV_HdmiTx_PioEnable(InstancePtr)
| This macro enables the HDMI TX PIO peripheral. More...
#define | XV_HdmiTx_PioDisable(InstancePtr)
| This macro disables the HDMI TX PIO peripheral. More...
#define | XV_HdmiTx_PioIntrEnable(InstancePtr)
| This macro enables interrupt in the HDMI TX PIO peripheral. More...
#define | XV_HdmiTx_PioIntrDisable(InstancePtr)
| This macro disables interrupt in the HDMI TX PIO peripheral. More...
#define | XV_HdmiTx_PioIntrClear(InstancePtr)
| This macro clears HDMI TX PIO interrupt. More...
#define | XV_HdmiTx_DdcEnable(InstancePtr)
| This macro enables the HDMI TX Display Data Channel (DDC) peripheral. More...
#define | XV_HdmiTx_DdcDisable(InstancePtr)
| This macro disables the HDMI TX Display Data Channel (DDC) peripheral. More...
#define | XV_HdmiTx_DdcIntrEnable(InstancePtr)
| This macro enables interrupt in the HDMI TX DDC peripheral. More...
#define | XV_HdmiTx_DdcIntrDisable(InstancePtr)
| This macro disables interrupt in the HDMI TX DDC peripheral. More...
#define | XV_HdmiTx_DdcIntrClear(InstancePtr)
| This macro clears HDMI TX DDC interrupt. More...
#define | XV_HdmiTx_AuxEnable(InstancePtr)
| This macro enables the HDMI TX Auxiliary (AUX) peripheral. More...
#define | XV_HdmiTx_AuxDisable(InstancePtr)
| This macro disables the HDMI TX Auxiliary (AUX) peripheral. More...
#define | XV_HdmiTx_AuxIntrEnable(InstancePtr)
| This macro enables interrupt in the HDMI TX AUX peripheral. More...
#define | XV_HdmiTx_AuxIntrDisable(InstancePtr)
| This macro disables interrupt in the HDMI TX AUX peripheral. More...
#define | XV_HdmiTx_AudioEnable(InstancePtr)
| This macro enables audio in HDMI TX core. More...
#define | XV_HdmiTx_AudioDisable(InstancePtr)
| This macro disables audio in HDMI TX core. More...
#define | XV_HdmiTx_AudioUnmute(InstancePtr)
| This macro unmutes audio in HDMI TX core. More...
#define | XV_HdmiTx_AudioMute(InstancePtr)
| This macro mutes audio in HDMI TX core. More...
#define | XV_HdmiTx_SetMode(InstancePtr)
| This macro sets the mode bit. More...
#define | XV_HdmiTx_ClearMode(InstancePtr)
| This macro clears the mode bit. More...
#define | XV_HdmiTx_GetMode(InstancePtr)
| This macro provides the current mode. More...
#define | XV_HdmiTx_GetSampleRate(InstancePtr) (InstancePtr)->Stream.SampleRate
| This macro provides the current sample rate. More...
#define | XV_HdmiTx_GetAudioChannels(InstancePtr) (InstancePtr)->Stream.Audio.Channels
| This macro provides the active audio channels. More...
#define | XV_HdmiTx_GetPixelPackingPhase(InstancePtr)
| This macro provides the current pixel packing phase. More...
#define | XV_HdmiTx_MaskDisable(InstancePtr)
| This macro disables video mask in HDMI TX core. More...
#define | XV_HdmiTx_MaskEnable(InstancePtr)
| This macro enables video mask in HDMI TX core. More...
#define | XV_HdmiTx_MaskNoise(InstancePtr, SetClr)
| This macro enables or disables the noise in the video mask. More...
#define | XV_HdmiTx_MaskSetRed(InstancePtr, Value)
| This macro sets the red component value in the video mask. More...
#define | XV_HdmiTx_MaskSetGreen(InstancePtr, Value)
| This macro sets the green component value in the video mask. More...
#define | XV_HdmiTx_MaskSetBlue(InstancePtr, Value)
| This macro sets the blue component value in the video mask. More...
#define | XV_HdmiTx_IsMasked(InstancePtr)
| This macro provides the current video mask mode. More...
enum | XV_HdmiTx_AudioFormatType
typedef void(* | XV_HdmiTx_Callback )(void *CallbackRef)
| Callback type for Vsync event interrupt. More...
XV_HdmiTx_Config * | XV_HdmiTx_LookupConfig (u16 DeviceId)
| This function returns a reference to an XV_HdmiTx_Config structure based on the core id, DeviceId. More...
int | XV_HdmiTx_CfgInitialize (XV_HdmiTx *InstancePtr, XV_HdmiTx_Config *CfgPtr, UINTPTR EffectiveAddr)
| This function initializes the HDMI TX core. More...
void | XV_HdmiTx_SetHdmiMode (XV_HdmiTx *InstancePtr)
| This function sets the core into HDMI mode. More...
void | XV_HdmiTx_SetDviMode (XV_HdmiTx *InstancePtr)
| This function sets the core into DVI mode. More...
void | XV_HdmiTx_Clear (XV_HdmiTx *InstancePtr)
| This function clear the HDMI TX variables and sets it to the defaults. More...
u8 | XV_HdmiTx_GetVic (XVidC_VideoMode VideoMode)
XVidC_VideoMode | XV_HdmiTx_GetVideoModeFromVic (u8 Vic)
u32 | XV_HdmiTx_SetStream (XV_HdmiTx *InstancePtr, XVidC_VideoMode VideoMode, XVidC_ColorFormat ColorFormat, XVidC_ColorDepth Bpc, XVidC_PixelsPerClock Ppc, XVidC_3DInfo *Info3D)
| This function sets the HDMI TX stream parameters. More...
u32 | XV_HdmiTx_GetTmdsClk (XV_HdmiTx *InstancePtr, XVidC_VideoMode VideoMode, XVidC_ColorFormat ColorFormat, XVidC_ColorDepth Bpc)
| This function sets and return the TMDS Clock based on Video Parameter. More...
void | XV_HdmiTx_INT_VRST (XV_HdmiTx *InstancePtr, u8 Reset)
| This function asserts or releases the HDMI TX Internal VRST. More...
void | XV_HdmiTx_INT_LRST (XV_HdmiTx *InstancePtr, u8 Reset)
| This function asserts or releases the HDMI TX Internal LRST. More...
void | XV_HdmiTx_EXT_VRST (XV_HdmiTx *InstancePtr, u8 Reset)
| This function asserts or releases the HDMI TX External VRST. More...
void | XV_HdmiTx_EXT_SYSRST (XV_HdmiTx *InstancePtr, u8 Reset)
| This function asserts or releases the HDMI TX External SYSRST. More...
void | XV_HdmiTx_SetGcpAvmuteBit (XV_HdmiTx *InstancePtr)
| This function sets the HDMI TX AUX GCP register AVMUTE bit. More...
void | XV_HdmiTx_ClearGcpAvmuteBit (XV_HdmiTx *InstancePtr)
| This function clears the HDMI TX AUX GCP register AVMUTE bit. More...
void | XV_HdmiTx_SetGcpClearAvmuteBit (XV_HdmiTx *InstancePtr)
| This function sets the HDMI TX AUX GCP register CLEAR_AVMUTE bit. More...
void | XV_HdmiTx_ClearGcpClearAvmuteBit (XV_HdmiTx *InstancePtr)
| This function clears the HDMI TX AUX GCP register CLEAR_AVMUTE bit. More...
void | XV_HdmiTx_SetPixelRate (XV_HdmiTx *InstancePtr)
| This function sets the pixel rate at output. More...
void | XV_HdmiTx_SetSampleRate (XV_HdmiTx *InstancePtr, u8 SampleRate)
| This function sets the sample rate at output. More...
void | XV_HdmiTx_SetColorFormat (XV_HdmiTx *InstancePtr)
| This function sets the color format. More...
void | XV_HdmiTx_SetColorDepth (XV_HdmiTx *InstancePtr)
| This function sets the color depth. More...
int | XV_HdmiTx_IsStreamScrambled (XV_HdmiTx *InstancePtr)
| This function provides status of the stream. More...
int | XV_HdmiTx_IsStreamConnected (XV_HdmiTx *InstancePtr)
| This function provides the stream connected status. More...
void | XV_HdmiTx_SetAxiClkFreq (XV_HdmiTx *InstancePtr, u32 ClkFreq)
| This function sets the AXI4-Lite Clock Frequency. More...
void | XV_HdmiTx_DdcInit (XV_HdmiTx *InstancePtr, u32 Frequency)
| This function prepares TX DDC peripheral to use. More...
int | XV_HdmiTx_DdcWrite (XV_HdmiTx *InstancePtr, u8 Slave, u16 Length, u8 *Buffer, u8 Stop)
| This function writes data from DDC peripheral from given slave address. More...
int | XV_HdmiTx_DdcRead (XV_HdmiTx *InstancePtr, u8 Slave, u16 Length, u8 *Buffer, u8 Stop)
| This function reads data from DDC peripheral from given slave address. More...
u32 | XV_HdmiTx_AuxSend (XV_HdmiTx *InstancePtr)
| This function transmits the infoframes generated by the processor. More...
int | XV_HdmiTx_Scrambler (XV_HdmiTx *InstancePtr)
| This function controls the scrambler. More...
int | XV_HdmiTx_ClockRatio (XV_HdmiTx *InstancePtr)
| This function controls the TMDS clock ratio. More...
int | XV_HdmiTx_DetectHdmi20 (XV_HdmiTx *InstancePtr)
| This function detects connected sink is a HDMI 2.0/HDMI 1.4 sink device and sets appropriate flag in the TX stream. More...
void | XV_HdmiTx_ShowSCDC (XV_HdmiTx *InstancePtr)
| This function shows the sinks SCDC registers. More...
void | XV_HdmiTx_DebugInfo (XV_HdmiTx *InstancePtr)
| This function prints stream and timing information on STDIO/Uart console. More...
int | XV_HdmiTx_SetAudioChannels (XV_HdmiTx *InstancePtr, u8 Value)
| This function sets the active audio channels. More...
int | XV_HdmiTx_SetAudioFormat (XV_HdmiTx *InstancePtr, XV_HdmiTx_AudioFormatType Value)
| This function sets the active audio format. More...
XV_HdmiTx_AudioFormatType | XV_HdmiTx_GetAudioFormat (XV_HdmiTx *InstancePtr)
| This function gets the active audio format. More...
int | XV_HdmiTx_SelfTest (XV_HdmiTx *InstancePtr)
| This function reads ID of HDMI TX PIO peripheral. More...
void | XV_HdmiTx_IntrHandler (void *InstancePtr)
| This function is the interrupt handler for the HDMI TX driver. More...
int | XV_HdmiTx_SetCallback (XV_HdmiTx *InstancePtr, XV_HdmiTx_HandlerType HandlerType, void *CallbackFunc, void *CallbackRef)
| This function installs an asynchronous callback function for the given HandlerType: More...
int | XV_HdmiTx_VSIF_GeneratePacket (XV_HdmiTx_VSIF *VSIFPtr, XHdmiC_Aux *AuxPtr)
| This function generates a Vendor Specific InfoFrame (VSIF). More...
void | XV_HdmiTx_VSIF_DisplayInfo (XV_HdmiTx_VSIF *VSIFPtr)
| This function displays the contents of an XV_HdmiTx_VSIF instance. More...
char * | XV_HdmiTx_VSIF_3DStructToString (XV_HdmiTx_3D_Struct_Field Item)
| This function returns a string representation of the enumerated type XV_HdmiTx_3D_Struct_Field. More...
char * | XV_HdmiTx_VSIF_3DSampMethodToString (XV_HdmiTx_3D_Sampling_Method Item)
| This function returns a string representation of the enumerated type XV_HdmiTx_3D_Sampling_Method. More...
char * | XV_HdmiTx_VSIF_3DSampPosToString (XV_HdmiTx_3D_Sampling_Position Item)
| This function returns a string representation of the enumerated type XV_HdmiTx_3D_Sampling_Position. More...

## Macro Definition Documentation

#define XV_HdmiTx_AudioDisable | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_AUD_CTRL_CLR_OFFSET), (XV_HDMITX_AUD_CTRL_RUN_MASK))
XV_HDMITX_AUD_CTRL_CLR_OFFSET
#define XV_HDMITX_AUD_CTRL_CLR_OFFSET
AUD Control Register Clear * offset.
Definition: xv_hdmitx_hw.h:341
XV_HDMITX_AUD_CTRL_RUN_MASK
#define XV_HDMITX_AUD_CTRL_RUN_MASK
AUD Control Run mask.
Definition: xv_hdmitx_hw.h:355
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456

This macro disables audio in HDMI TX core.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_AudioDisable(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_CfgInitialize(), and XV_HdmiTx_SetDviMode().

#define XV_HdmiTx_AudioEnable | ( |  | InstancePtr | ) |

Value:
{ \
if ((InstancePtr)->Stream.IsHdmi) { \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_AUD_CTRL_SET_OFFSET), (XV_HDMITX_AUD_CTRL_RUN_MASK)); \
} \
}
XV_HDMITX_AUD_CTRL_RUN_MASK
#define XV_HDMITX_AUD_CTRL_RUN_MASK
AUD Control Run mask.
Definition: xv_hdmitx_hw.h:355
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_AUD_CTRL_SET_OFFSET
#define XV_HDMITX_AUD_CTRL_SET_OFFSET
AUD Control Register Set * offset.
Definition: xv_hdmitx_hw.h:338

This macro enables audio in HDMI TX core.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_AudioEnable(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_SetHdmiMode().

#define XV_HdmiTx_AudioMute | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_AUD_CTRL_CLR_OFFSET), (XV_HDMITX_AUD_CTRL_RUN_MASK)) \
_Pragma ("GCC warning \"'XV_HdmiTx_AudioMute' macro is deprecated\"")
XV_HDMITX_AUD_CTRL_CLR_OFFSET
#define XV_HDMITX_AUD_CTRL_CLR_OFFSET
AUD Control Register Clear * offset.
Definition: xv_hdmitx_hw.h:341
XV_HDMITX_AUD_CTRL_RUN_MASK
#define XV_HDMITX_AUD_CTRL_RUN_MASK
AUD Control Run mask.
Definition: xv_hdmitx_hw.h:355
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456

This macro mutes audio in HDMI TX core.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_AudioMute(XV_HdmiTx *InstancePtr)

#define XV_HdmiTx_AudioUnmute | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_AUD_CTRL_SET_OFFSET), (XV_HDMITX_AUD_CTRL_RUN_MASK)) \
_Pragma ("GCC warning \"'XV_HdmiTx_AudioUnmute' macro is deprecated\"")
XV_HDMITX_AUD_CTRL_RUN_MASK
#define XV_HDMITX_AUD_CTRL_RUN_MASK
AUD Control Run mask.
Definition: xv_hdmitx_hw.h:355
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_AUD_CTRL_SET_OFFSET
#define XV_HDMITX_AUD_CTRL_SET_OFFSET
AUD Control Register Set * offset.
Definition: xv_hdmitx_hw.h:338

This macro unmutes audio in HDMI TX core.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_AudioUnmute(XV_HdmiTx *InstancePtr)

#define XV_HdmiTx_AuxDisable | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_AUX_CTRL_CLR_OFFSET), (XV_HDMITX_AUX_CTRL_RUN_MASK))
XV_HDMITX_AUX_CTRL_RUN_MASK
#define XV_HDMITX_AUX_CTRL_RUN_MASK
AUX Control Run mask.
Definition: xv_hdmitx_hw.h:303
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_AUX_CTRL_CLR_OFFSET
#define XV_HDMITX_AUX_CTRL_CLR_OFFSET
AUX Control Register Clear * offset.
Definition: xv_hdmitx_hw.h:292

This macro disables the HDMI TX Auxiliary (AUX) peripheral.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_AuxDisable(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_CfgInitialize(), and XV_HdmiTx_SetDviMode().

#define XV_HdmiTx_AuxEnable | ( |  | InstancePtr | ) |

Value:
{ \
if ((InstancePtr)->Stream.IsHdmi) { \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_AUX_CTRL_SET_OFFSET), (XV_HDMITX_AUX_CTRL_RUN_MASK)); \
} \
}
XV_HDMITX_AUX_CTRL_RUN_MASK
#define XV_HDMITX_AUX_CTRL_RUN_MASK
AUX Control Run mask.
Definition: xv_hdmitx_hw.h:303
XV_HDMITX_AUX_CTRL_SET_OFFSET
#define XV_HDMITX_AUX_CTRL_SET_OFFSET
AUX Control Register Set * offset.
Definition: xv_hdmitx_hw.h:289
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456

This macro enables the HDMI TX Auxiliary (AUX) peripheral.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_AuxEnable(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_SetHdmiMode().

#define XV_HdmiTx_AuxIntrDisable | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_AUX_CTRL_CLR_OFFSET), (XV_HDMITX_AUX_CTRL_IE_MASK))
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_AUX_CTRL_CLR_OFFSET
#define XV_HDMITX_AUX_CTRL_CLR_OFFSET
AUX Control Register Clear * offset.
Definition: xv_hdmitx_hw.h:292
XV_HDMITX_AUX_CTRL_IE_MASK
#define XV_HDMITX_AUX_CTRL_IE_MASK
AUX Control Interrupt Enable mask.
Definition: xv_hdmitx_hw.h:304

This macro disables interrupt in the HDMI TX AUX peripheral.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_AuxIntrDisable(XV_HdmiTx *InstancePtr)

#define XV_HdmiTx_AuxIntrEnable | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_AUX_CTRL_SET_OFFSET), (XV_HDMITX_AUX_CTRL_IE_MASK))
XV_HDMITX_AUX_CTRL_SET_OFFSET
#define XV_HDMITX_AUX_CTRL_SET_OFFSET
AUX Control Register Set * offset.
Definition: xv_hdmitx_hw.h:289
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_AUX_CTRL_IE_MASK
#define XV_HDMITX_AUX_CTRL_IE_MASK
AUX Control Interrupt Enable mask.
Definition: xv_hdmitx_hw.h:304

This macro enables interrupt in the HDMI TX AUX peripheral.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_AuxIntrEnable(XV_HdmiTx *InstancePtr)

#define XV_HdmiTx_Bridge_pixel | ( |  | InstancePtr,
|  |  | SetClr
| ) |  |

Value:
{ \
if (SetClr) { \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_OUT_SET_OFFSET), \
(XV_HDMITX_PIO_OUT_BRIDGE_PIXEL_MASK)); \
} \
else { \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_OUT_CLR_OFFSET), \
(XV_HDMITX_PIO_OUT_BRIDGE_PIXEL_MASK)); \
} \
}
XV_HDMITX_PIO_OUT_SET_OFFSET
#define XV_HDMITX_PIO_OUT_SET_OFFSET
PIO Out Register Set * offset.
Definition: xv_hdmitx_hw.h:89
XV_HDMITX_PIO_OUT_CLR_OFFSET
#define XV_HDMITX_PIO_OUT_CLR_OFFSET
PIO Out Register Clear * offset.
Definition: xv_hdmitx_hw.h:92
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_PIO_OUT_BRIDGE_PIXEL_MASK
#define XV_HDMITX_PIO_OUT_BRIDGE_PIXEL_MASK
PIO Out Bridge_Pixel repeat mask.
Definition: xv_hdmitx_hw.h:170

This macro controls the Pixel Repeat mode for video bridge.

Parameters

  InstancePtr | is a pointer to the XHdmi_Tx core instance.
  SetClr | specifies TRUE/FALSE value to either enable or disable the Pixel Repitition Support.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_Bridge_pixel(XV_HdmiTx *InstancePtr, u8 SetClr)

#define XV_HdmiTx_Bridge_yuv420 | ( |  | InstancePtr,
|  |  | SetClr
| ) |  |

Value:
{ \
if (SetClr) { \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_OUT_SET_OFFSET), \
(XV_HDMITX_PIO_OUT_BRIDGE_YUV420_MASK)); \
} \
else { \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_OUT_CLR_OFFSET), \
(XV_HDMITX_PIO_OUT_BRIDGE_YUV420_MASK)); \
} \
}
XV_HDMITX_PIO_OUT_BRIDGE_YUV420_MASK
#define XV_HDMITX_PIO_OUT_BRIDGE_YUV420_MASK
PIO Out Bridge_YUV420 mask.
Definition: xv_hdmitx_hw.h:167
XV_HDMITX_PIO_OUT_SET_OFFSET
#define XV_HDMITX_PIO_OUT_SET_OFFSET
PIO Out Register Set * offset.
Definition: xv_hdmitx_hw.h:89
XV_HDMITX_PIO_OUT_CLR_OFFSET
#define XV_HDMITX_PIO_OUT_CLR_OFFSET
PIO Out Register Clear * offset.
Definition: xv_hdmitx_hw.h:92
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456

This macro controls the YUV420 mode for video bridge.

Parameters

  InstancePtr | is a pointer to the XHdmi_Tx core instance.
  SetClr | specifies TRUE/FALSE value to either enable or disable the YUV 420 Support.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_Bridge_yuv420(XV_HdmiTx *InstancePtr, u8 SetClr)

#define XV_HdmiTx_ClearMode | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_OUT_CLR_OFFSET), (XV_HDMITX_PIO_OUT_MODE_MASK))
XV_HDMITX_PIO_OUT_MODE_MASK
#define XV_HDMITX_PIO_OUT_MODE_MASK
PIO Out Mode mask.
Definition: xv_hdmitx_hw.h:136
XV_HDMITX_PIO_OUT_CLR_OFFSET
#define XV_HDMITX_PIO_OUT_CLR_OFFSET
PIO Out Register Clear * offset.
Definition: xv_hdmitx_hw.h:92
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456

This macro clears the mode bit.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_ClearMode(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_SetDviMode().

#define XV_HdmiTx_DdcDisable | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_DDC_CTRL_CLR_OFFSET), (XV_HDMITX_DDC_CTRL_RUN_MASK))
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_DDC_CTRL_RUN_MASK
#define XV_HDMITX_DDC_CTRL_RUN_MASK
DDC Control Run mask.
Definition: xv_hdmitx_hw.h:244
XV_HDMITX_DDC_CTRL_CLR_OFFSET
#define XV_HDMITX_DDC_CTRL_CLR_OFFSET
DDC Control Register Clear * offset.
Definition: xv_hdmitx_hw.h:230

This macro disables the HDMI TX Display Data Channel (DDC) peripheral.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_DdcDisable(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_CfgInitialize(), XV_HdmiTx_DdcRead(), and XV_HdmiTx_DdcWrite().

#define XV_HdmiTx_DdcEnable | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_DDC_CTRL_SET_OFFSET), (XV_HDMITX_DDC_CTRL_RUN_MASK))
XV_HDMITX_DDC_CTRL_SET_OFFSET
#define XV_HDMITX_DDC_CTRL_SET_OFFSET
DDC Control Register Set * offset.
Definition: xv_hdmitx_hw.h:227
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_DDC_CTRL_RUN_MASK
#define XV_HDMITX_DDC_CTRL_RUN_MASK
DDC Control Run mask.
Definition: xv_hdmitx_hw.h:244

This macro enables the HDMI TX Display Data Channel (DDC) peripheral.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_DdcEnable(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_DdcRead(), and XV_HdmiTx_DdcWrite().

#define XV_HdmiTx_DdcIntrClear | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_DDC_STA_OFFSET), (XV_HDMITX_DDC_STA_IRQ_MASK))
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_DDC_STA_OFFSET
#define XV_HDMITX_DDC_STA_OFFSET
DDC Status Register * offset.
Definition: xv_hdmitx_hw.h:233
XV_HDMITX_DDC_STA_IRQ_MASK
#define XV_HDMITX_DDC_STA_IRQ_MASK
DDC Status IRQ mask.
Definition: xv_hdmitx_hw.h:255

This macro clears HDMI TX DDC interrupt.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_DdcIntrClear(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_CfgInitialize().

#define XV_HdmiTx_DdcIntrDisable | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_DDC_CTRL_CLR_OFFSET), (XV_HDMITX_DDC_CTRL_IE_MASK))
XV_HDMITX_DDC_CTRL_IE_MASK
#define XV_HDMITX_DDC_CTRL_IE_MASK
DDC Control Interrupt Enable mask.
Definition: xv_hdmitx_hw.h:245
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_DDC_CTRL_CLR_OFFSET
#define XV_HDMITX_DDC_CTRL_CLR_OFFSET
DDC Control Register Clear * offset.
Definition: xv_hdmitx_hw.h:230

This macro disables interrupt in the HDMI TX DDC peripheral.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_DdcIntrDisable(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_DdcRead(), and XV_HdmiTx_DdcWrite().

#define XV_HdmiTx_DdcIntrEnable | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_DDC_CTRL_SET_OFFSET), (XV_HDMITX_DDC_CTRL_IE_MASK))
XV_HDMITX_DDC_CTRL_SET_OFFSET
#define XV_HDMITX_DDC_CTRL_SET_OFFSET
DDC Control Register Set * offset.
Definition: xv_hdmitx_hw.h:227
XV_HDMITX_DDC_CTRL_IE_MASK
#define XV_HDMITX_DDC_CTRL_IE_MASK
DDC Control Interrupt Enable mask.
Definition: xv_hdmitx_hw.h:245
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456

This macro enables interrupt in the HDMI TX DDC peripheral.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_DdcIntrEnable(XV_HdmiTx *InstancePtr)

#define XV_HdmiTx_GetAudioChannels | ( |  | InstancePtr | ) | (InstancePtr)->Stream.Audio.Channels

This macro provides the active audio channels.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  Audio channels

#define XV_HdmiTx_GetMode | ( |  | InstancePtr | ) |

Value:
(XV_HdmiTx_ReadReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_OUT_OFFSET)) & (XV_HDMITX_PIO_OUT_MODE_MASK))
XV_HDMITX_PIO_OUT_MODE_MASK
#define XV_HDMITX_PIO_OUT_MODE_MASK
PIO Out Mode mask.
Definition: xv_hdmitx_hw.h:136
XV_HdmiTx_ReadReg
#define XV_HdmiTx_ReadReg(BaseAddress, RegOffset)
This macro reads a value from a HDMI TX register.
Definition: xv_hdmitx_hw.h:435
XV_HDMITX_PIO_OUT_OFFSET
#define XV_HDMITX_PIO_OUT_OFFSET
PIO Out Register offset.
Definition: xv_hdmitx_hw.h:86

This macro provides the current mode.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  Current mode. 0 = DVI 1 = HDMI

Note
  C-style signature: u8 XV_HdmiTx_GetMode(XV_HdmiTx *InstancePtr)

#define XV_HdmiTx_GetPixelPackingPhase | ( |  | InstancePtr | ) |

Value:
( ( (XV_HdmiTx_ReadReg( (InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_IN_OFFSET) ) ) >> (XV_HDMITX_PIO_IN_PPP_SHIFT)) \
& (XV_HDMITX_PIO_IN_PPP_MASK))
XV_HdmiTx_ReadReg
#define XV_HdmiTx_ReadReg(BaseAddress, RegOffset)
This macro reads a value from a HDMI TX register.
Definition: xv_hdmitx_hw.h:435
XV_HDMITX_PIO_IN_OFFSET
#define XV_HDMITX_PIO_IN_OFFSET
PIO In Register offset.
Definition: xv_hdmitx_hw.h:98
XV_HDMITX_PIO_IN_PPP_SHIFT
#define XV_HDMITX_PIO_IN_PPP_SHIFT
PIO In Pixel packing phase shift.
Definition: xv_hdmitx_hw.h:205
XV_HDMITX_PIO_IN_PPP_MASK
#define XV_HDMITX_PIO_IN_PPP_MASK
PIO In Pixel packing phase mask.
Definition: xv_hdmitx_hw.h:199

This macro provides the current pixel packing phase.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  Pixel packing phase.

#define XV_HdmiTx_GetSampleRate | ( |  | InstancePtr | ) | (InstancePtr)->Stream.SampleRate

This macro provides the current sample rate.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  Sample rate

Note
  C-style signature: u8 XV_HdmiTx_GetSampleRate(XV_HdmiTx *InstancePtr)

#define XV_HdmiTx_GetTime1Ms | ( |  | InstancePtr | ) | (InstancePtr)->Config.AxiLiteClkFreq/1000

This macro returns the clock cycles required to count up to 1MS with respect to AXI Lite Frequency.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTX core instance.

Returns
  None.

Referenced by XV_HdmiTx_CfgInitialize().

#define XV_HdmiTx_GetVersion | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_ReadReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_VER_VERSION_OFFSET))
XV_HdmiTx_ReadReg
#define XV_HdmiTx_ReadReg(BaseAddress, RegOffset)
This macro reads a value from a HDMI TX register.
Definition: xv_hdmitx_hw.h:435
XV_HDMITX_VER_VERSION_OFFSET
#define XV_HDMITX_VER_VERSION_OFFSET
VER Version Register * offset.
Definition: xv_hdmitx_hw.h:64

This macro reads the TX version.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTX core instance.

Returns
  None.

#define XV_HDMITX_H_

Prevent circular inclusions by using protection macros.

#define XV_HdmiTx_IsMasked | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_ReadReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_MASK_CTRL_OFFSET)) & (XV_HDMITX_MASK_CTRL_RUN_MASK)
XV_HDMITX_MASK_CTRL_OFFSET
#define XV_HDMITX_MASK_CTRL_OFFSET
MASK Control Register * offset.
Definition: xv_hdmitx_hw.h:377
XV_HdmiTx_ReadReg
#define XV_HdmiTx_ReadReg(BaseAddress, RegOffset)
This macro reads a value from a HDMI TX register.
Definition: xv_hdmitx_hw.h:435
XV_HDMITX_MASK_CTRL_RUN_MASK
#define XV_HDMITX_MASK_CTRL_RUN_MASK
MASK Control Run mask.
Definition: xv_hdmitx_hw.h:400

This macro provides the current video mask mode.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  Current mode. 0 = Video masking is disabled 1 = Video masking is enabled

Note
  C-style signature: u8 XV_HdmiTx_IsMasked(XV_HdmiTx *InstancePtr)

#define XV_HdmiTx_MaskDisable | ( |  | InstancePtr | ) |

Value:
{ \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_MASK_CTRL_CLR_OFFSET), (XV_HDMITX_MASK_CTRL_RUN_MASK)); \
}
XV_HDMITX_MASK_CTRL_CLR_OFFSET
#define XV_HDMITX_MASK_CTRL_CLR_OFFSET
MASK Control Register Clear * offset.
Definition: xv_hdmitx_hw.h:383
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_MASK_CTRL_RUN_MASK
#define XV_HDMITX_MASK_CTRL_RUN_MASK
MASK Control Run mask.
Definition: xv_hdmitx_hw.h:400

This macro disables video mask in HDMI TX core.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_MaskDisable(XV_HdmiTx *InstancePtr)

#define XV_HdmiTx_MaskEnable | ( |  | InstancePtr | ) |

Value:
{ \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_MASK_CTRL_SET_OFFSET), (XV_HDMITX_MASK_CTRL_RUN_MASK)); \
}
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_MASK_CTRL_SET_OFFSET
#define XV_HDMITX_MASK_CTRL_SET_OFFSET
MASK Control Register Set * offset.
Definition: xv_hdmitx_hw.h:380
XV_HDMITX_MASK_CTRL_RUN_MASK
#define XV_HDMITX_MASK_CTRL_RUN_MASK
MASK Control Run mask.
Definition: xv_hdmitx_hw.h:400

This macro enables video mask in HDMI TX core.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_MaskEnable(XV_HdmiTx *InstancePtr)

#define XV_HdmiTx_MaskNoise | ( |  | InstancePtr,
|  |  | SetClr
| ) |  |

Value:
{ \
if (SetClr) { \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_MASK_CTRL_SET_OFFSET), \
(XV_HDMITX_MASK_CTRL_NOISE_MASK)); \
} \
else { \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_MASK_CTRL_CLR_OFFSET), \
(XV_HDMITX_MASK_CTRL_NOISE_MASK)); \
} \
}
XV_HDMITX_MASK_CTRL_CLR_OFFSET
#define XV_HDMITX_MASK_CTRL_CLR_OFFSET
MASK Control Register Clear * offset.
Definition: xv_hdmitx_hw.h:383
XV_HDMITX_MASK_CTRL_NOISE_MASK
#define XV_HDMITX_MASK_CTRL_NOISE_MASK
MASK Control Noise.
Definition: xv_hdmitx_hw.h:401
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_MASK_CTRL_SET_OFFSET
#define XV_HDMITX_MASK_CTRL_SET_OFFSET
MASK Control Register Set * offset.
Definition: xv_hdmitx_hw.h:380

This macro enables or disables the noise in the video mask.

Parameters

  InstancePtr | is a pointer to the XHdmi_Tx core instance.
  SetClr | specifies TRUE/FALSE value to either enable or disable the Noise.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_MaskNoise(XV_HdmiTx *InstancePtr, u8 SetClr)

#define XV_HdmiTx_MaskSetBlue | ( |  | InstancePtr,
|  |  | Value
| ) |  |

Value:
{ \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_MASK_BLUE_OFFSET), \
(Value)); \
}
XV_HDMITX_MASK_BLUE_OFFSET
#define XV_HDMITX_MASK_BLUE_OFFSET
MASK Blue Component Register * offset.
Definition: xv_hdmitx_hw.h:395
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456

This macro sets the blue component value in the video mask.

Parameters

  InstancePtr | is a pointer to the XHdmi_Tx core instance.
  Value |

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_MaskSetBlue(XV_HdmiTx *InstancePtr, u16 Value)

#define XV_HdmiTx_MaskSetGreen | ( |  | InstancePtr,
|  |  | Value
| ) |  |

Value:
{ \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_MASK_GREEN_OFFSET), \
(Value)); \
}
XV_HDMITX_MASK_GREEN_OFFSET
#define XV_HDMITX_MASK_GREEN_OFFSET
MASK Green Component Register * offset.
Definition: xv_hdmitx_hw.h:392
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456

This macro sets the green component value in the video mask.

Parameters

  InstancePtr | is a pointer to the XHdmi_Tx core instance.
  Value |

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_MaskSetGreen(XV_HdmiTx *InstancePtr, u16 Value)

#define XV_HdmiTx_MaskSetRed | ( |  | InstancePtr,
|  |  | Value
| ) |  |

Value:
{ \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_MASK_RED_OFFSET), \
(Value)); \
}
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_MASK_RED_OFFSET
#define XV_HDMITX_MASK_RED_OFFSET
MASK Red Component Register * offset.
Definition: xv_hdmitx_hw.h:389

This macro sets the red component value in the video mask.

Parameters

  InstancePtr | is a pointer to the XHdmi_Tx core instance.
  Value |

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_MaskSetRed(XV_HdmiTx *InstancePtr, u16 Value)

#define XV_HdmiTx_PioDisable | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_CTRL_CLR_OFFSET), (XV_HDMITX_PIO_CTRL_RUN_MASK))
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_PIO_CTRL_RUN_MASK
#define XV_HDMITX_PIO_CTRL_RUN_MASK
PIO Control Run mask.
Definition: xv_hdmitx_hw.h:125
XV_HDMITX_PIO_CTRL_CLR_OFFSET
#define XV_HDMITX_PIO_CTRL_CLR_OFFSET
PIO Control Register Clear * offset.
Definition: xv_hdmitx_hw.h:80

This macro disables the HDMI TX PIO peripheral.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_PioDisable(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_CfgInitialize().

#define XV_HdmiTx_PioEnable | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_CTRL_SET_OFFSET), (XV_HDMITX_PIO_CTRL_RUN_MASK))
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_PIO_CTRL_RUN_MASK
#define XV_HDMITX_PIO_CTRL_RUN_MASK
PIO Control Run mask.
Definition: xv_hdmitx_hw.h:125
XV_HDMITX_PIO_CTRL_SET_OFFSET
#define XV_HDMITX_PIO_CTRL_SET_OFFSET
PIO Control Register Set * offset.
Definition: xv_hdmitx_hw.h:77

This macro enables the HDMI TX PIO peripheral.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_PioEnable(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_CfgInitialize().

#define XV_HdmiTx_PioIntrClear | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_STA_OFFSET), (XV_HDMITX_PIO_STA_IRQ_MASK))
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_PIO_STA_OFFSET
#define XV_HDMITX_PIO_STA_OFFSET
PIO Status Register * offset.
Definition: xv_hdmitx_hw.h:83
XV_HDMITX_PIO_STA_IRQ_MASK
#define XV_HDMITX_PIO_STA_IRQ_MASK
PIO Status Interrupt mask.
Definition: xv_hdmitx_hw.h:131

This macro clears HDMI TX PIO interrupt.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_PioIntrClear(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_CfgInitialize().

#define XV_HdmiTx_PioIntrDisable | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_CTRL_CLR_OFFSET), (XV_HDMITX_PIO_CTRL_IE_MASK))
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_PIO_CTRL_IE_MASK
#define XV_HDMITX_PIO_CTRL_IE_MASK
PIO Control Interrupt Enable mask.
Definition: xv_hdmitx_hw.h:126
XV_HDMITX_PIO_CTRL_CLR_OFFSET
#define XV_HDMITX_PIO_CTRL_CLR_OFFSET
PIO Control Register Clear * offset.
Definition: xv_hdmitx_hw.h:80

This macro disables interrupt in the HDMI TX PIO peripheral.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_PioIntrDisable(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_DdcRead(), and XV_HdmiTx_DdcWrite().

#define XV_HdmiTx_PioIntrEnable | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_CTRL_SET_OFFSET), (XV_HDMITX_PIO_CTRL_IE_MASK))
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_PIO_CTRL_IE_MASK
#define XV_HDMITX_PIO_CTRL_IE_MASK
PIO Control Interrupt Enable mask.
Definition: xv_hdmitx_hw.h:126
XV_HDMITX_PIO_CTRL_SET_OFFSET
#define XV_HDMITX_PIO_CTRL_SET_OFFSET
PIO Control Register Set * offset.
Definition: xv_hdmitx_hw.h:77

This macro enables interrupt in the HDMI TX PIO peripheral.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_PioIntrEnable(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_CfgInitialize(), XV_HdmiTx_DdcRead(), and XV_HdmiTx_DdcWrite().

#define XV_HdmiTx_Reset | ( |  | InstancePtr,
|  |  | Reset
| ) |  |

Value:
{ \
if (Reset) { \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_OUT_CLR_OFFSET), (XV_HDMITX_PIO_OUT_RST_MASK)); \
} \
else { \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_OUT_SET_OFFSET), (XV_HDMITX_PIO_OUT_RST_MASK)); \
} \
}
XV_HDMITX_PIO_OUT_SET_OFFSET
#define XV_HDMITX_PIO_OUT_SET_OFFSET
PIO Out Register Set * offset.
Definition: xv_hdmitx_hw.h:89
XV_HDMITX_PIO_OUT_CLR_OFFSET
#define XV_HDMITX_PIO_OUT_CLR_OFFSET
PIO Out Register Clear * offset.
Definition: xv_hdmitx_hw.h:92
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_PIO_OUT_RST_MASK
#define XV_HDMITX_PIO_OUT_RST_MASK
PIO Out Reset mask.
Definition: xv_hdmitx_hw.h:135

This macro asserts or releases the HDMI TX reset.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.
  Reset | specifies TRUE/FALSE value to either assert or release HDMI TX reset.

Returns
  None.

Note
  The reset output of the PIO is inverted. When the system is in reset, the PIO output is cleared and this will reset the HDMI RX. Therefore, clearing the PIO reset output will assert the HDMI link and video reset. C-style signature: void XV_HdmiTx_Reset(XV_HdmiTx *InstancePtr, u8 Reset)

#define XV_HdmiTx_SetMode | ( |  | InstancePtr | ) |

Value:
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_OUT_SET_OFFSET), (XV_HDMITX_PIO_OUT_MODE_MASK))
XV_HDMITX_PIO_OUT_MODE_MASK
#define XV_HDMITX_PIO_OUT_MODE_MASK
PIO Out Mode mask.
Definition: xv_hdmitx_hw.h:136
XV_HDMITX_PIO_OUT_SET_OFFSET
#define XV_HDMITX_PIO_OUT_SET_OFFSET
PIO Out Register Set * offset.
Definition: xv_hdmitx_hw.h:89
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456

This macro sets the mode bit.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_SetMode(XV_HdmiTx *InstancePtr)

Referenced by XV_HdmiTx_SetHdmiMode().

#define XV_HdmiTx_SetScrambler | ( |  | InstancePtr,
|  |  | SetClr
| ) |  |

Value:
{ \
if (SetClr) { \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_OUT_SET_OFFSET), (XV_HDMITX_PIO_OUT_SCRM_MASK)); \
(InstancePtr)->Stream.IsScrambled = (TRUE); \
} \
else { \
XV_HdmiTx_WriteReg((InstancePtr)->Config.BaseAddress, \
(XV_HDMITX_PIO_OUT_CLR_OFFSET), (XV_HDMITX_PIO_OUT_SCRM_MASK)); \
(InstancePtr)->Stream.IsScrambled = (FALSE); \
} \
}
XV_HDMITX_PIO_OUT_SET_OFFSET
#define XV_HDMITX_PIO_OUT_SET_OFFSET
PIO Out Register Set * offset.
Definition: xv_hdmitx_hw.h:89
XV_HDMITX_PIO_OUT_CLR_OFFSET
#define XV_HDMITX_PIO_OUT_CLR_OFFSET
PIO Out Register Clear * offset.
Definition: xv_hdmitx_hw.h:92
XV_HdmiTx_WriteReg
#define XV_HdmiTx_WriteReg(BaseAddress, RegOffset, Data)
This macro writes a value to a HDMI TX register.
Definition: xv_hdmitx_hw.h:456
XV_HDMITX_PIO_OUT_SCRM_MASK
#define XV_HDMITX_PIO_OUT_SCRM_MASK
PIO Out Scrambler mask.
Definition: xv_hdmitx_hw.h:149

This macro controls the HDMI TX Scrambler.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.
  SetClr | specifies TRUE/FALSE value to either set ON or clear Scrambler.

Returns
  None.

Note
  C-style signature: void XV_HdmiTx_SetScrambler(XV_HdmiTx *InstancePtr, u8 SetClr)

Referenced by XV_HdmiTx_Scrambler().

## Typedef Documentation

typedef void(* XV_HdmiTx_Callback)(void *CallbackRef)

Callback type for Vsync event interrupt.

Parameters

  CallbackRef | is a callback reference passed in by the upper layer when setting the callback functions, and passed back to the upper layer when the callback is invoked.

Returns
  None.

Note
  None.

## Enumeration Type Documentation

enum XV_HdmiTx_HandlerType

These constants specify different types of handler and used to differentiate interrupt requests from peripheral.

## Function Documentation

u32 XV_HdmiTx_AuxSend | ( | XV_HdmiTx * | InstancePtr | ) |

This function transmits the infoframes generated by the processor.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  - XST_SUCCESS if infoframes transmitted successfully.
  - XST_FAILURE if AUX FIFO is full.

Note
  None.

References XV_HdmiTx::Aux, XV_HdmiTx_Config::BaseAddress, XV_HdmiTx::Config, XV_HDMITX_AUX_DAT_OFFSET, XV_HDMITX_AUX_STA_FIFO_FUL_MASK, XV_HDMITX_AUX_STA_OFFSET, XV_HDMITX_AUX_STA_PKT_RDY_MASK, XV_HdmiTx_ReadReg, and XV_HdmiTx_WriteReg.

int XV_HdmiTx_CfgInitialize | ( | XV_HdmiTx * | InstancePtr,
|  | XV_HdmiTx_Config * | CfgPtr,
|  | UINTPTR | EffectiveAddr
| ) |  |

This function initializes the HDMI TX core.

This function must be called prior to using the HDMI TX core. Initialization of the HDMI TX includes setting up the instance data and ensuring the hardware is in a quiescent state.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.
  CfgPtr | points to the configuration structure associated with the HDMI TX core.
  EffectiveAddr | is the base address of the device. If address translation is being used, then this parameter must reflect the virtual base address. Otherwise, the physical address should be used.

Returns
  - XST_SUCCESS if XV_HdmiTx_CfgInitialize was successful.
  - XST_FAILURE if HDMI TX PIO ID mismatched.

Note
  None.

References XV_HdmiTx_Config::BaseAddress, XV_HdmiTx::Config, XV_HdmiTx::ConnectCallback, XV_HdmiTx::IsConnectCallbackSet, XV_HdmiTx_Stream::IsConnected, XV_HdmiTx::IsReady, XV_HdmiTx::IsStreamDownCallbackSet, XV_HdmiTx::IsStreamUpCallbackSet, XV_HdmiTx::IsToggleCallbackSet, XV_HdmiTx::IsVsCallbackSet, XV_HdmiTx_Stream::OverrideScrambler, XV_HdmiTx_Stream::State, XV_HdmiTx::Stream, XV_HdmiTx::StreamDownCallback, XV_HdmiTx::StreamUpCallback, XV_HdmiTx::ToggleCallback, XV_HdmiTx::VsCallback, XV_HdmiTx_AudioDisable, XV_HdmiTx_AuxDisable, XV_HdmiTx_Clear(), XV_HDMITX_CONNECT_CONF_OFFSET, XV_HdmiTx_DdcDisable, XV_HdmiTx_DdcIntrClear, XV_HdmiTx_GetTime1Ms, XV_HDMITX_HPD_TIMEGRID_OFFSET, XV_HDMITX_MASK_16, XV_HDMITX_PIO_ID, XV_HDMITX_PIO_ID_OFFSET, XV_HDMITX_PIO_IN_BRDG_LOCKED_MASK, XV_HDMITX_PIO_IN_BRDG_OVERFLOW_MASK, XV_HDMITX_PIO_IN_BRDG_UNDERFLOW_MASK, XV_HDMITX_PIO_IN_EVT_FE_OFFSET, XV_HDMITX_PIO_IN_EVT_RE_OFFSET, XV_HDMITX_PIO_IN_HPD_MASK, XV_HDMITX_PIO_IN_HPD_TOGGLE_MASK, XV_HDMITX_PIO_IN_LNK_RDY_MASK, XV_HDMITX_PIO_IN_VS_MASK, XV_HdmiTx_PioDisable, XV_HdmiTx_PioEnable, XV_HdmiTx_PioIntrClear, XV_HdmiTx_PioIntrEnable, XV_HdmiTx_ReadReg, XV_HdmiTx_SetHdmiMode(), XV_HDMITX_SHIFT_16, XV_HDMITX_TOGGLE_CONF_OFFSET, and XV_HdmiTx_WriteReg.

void XV_HdmiTx_Clear | ( | XV_HdmiTx * | InstancePtr | ) |

This function clear the HDMI TX variables and sets it to the defaults.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns

Note
  This is required after a reset or init.

Referenced by XV_HdmiTx_CfgInitialize().

void XV_HdmiTx_ClearGcpAvmuteBit | ( | XV_HdmiTx * | InstancePtr | ) |

This function clears the HDMI TX AUX GCP register AVMUTE bit.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  None.

References XV_HDMITX_PIO_OUT_CLR_OFFSET, XV_HDMITX_PIO_OUT_GCP_AVMUTE_MASK, and XV_HdmiTx_WriteReg.

void XV_HdmiTx_ClearGcpClearAvmuteBit | ( | XV_HdmiTx * | InstancePtr | ) |

This function clears the HDMI TX AUX GCP register CLEAR_AVMUTE bit.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  None.

References XV_HDMITX_PIO_OUT_CLR_OFFSET, XV_HDMITX_PIO_OUT_GCP_CLEARAVMUTE_MASK, and XV_HdmiTx_WriteReg.

int XV_HdmiTx_ClockRatio | ( | XV_HdmiTx * | InstancePtr | ) |

This function controls the TMDS clock ratio.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  - XST_SUCCESS if HDMI 2.0
  - XST_FAILURE if HDMI 1.4

Note
  None.

References XV_HdmiTx_Stream::IsHdmi20, XV_HdmiTx::Stream, XV_HdmiTx_Stream::TMDSClockRatio, XV_HdmiTx_DdcRead(), and XV_HdmiTx_DdcWrite().

Referenced by XV_HdmiTx_SetStream().

void XV_HdmiTx_DdcInit | ( | XV_HdmiTx * | InstancePtr,
|  | u32 | Frequency
| ) |  |

This function prepares TX DDC peripheral to use.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.
  Frequency | specifies the value that needs to be set.

Returns
  None.

Note
  None.

References XV_HdmiTx_Config::BaseAddress, XV_HdmiTx::Config, XV_HDMITX_DDC_CTRL_CLK_DIV_MASK, XV_HDMITX_DDC_CTRL_OFFSET, and XV_HdmiTx_WriteReg.

Referenced by XV_HdmiTx_SetAxiClkFreq().

int XV_HdmiTx_DdcRead | ( | XV_HdmiTx * | InstancePtr,
|  | u8 | Slave,
|  | u16 | Length,
|  | u8 * | Buffer,
|  | u8 | Stop
| ) |  |

This function reads data from DDC peripheral from given slave address.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.
  Slave | specifies the slave address from where data needs to be read.
  Length | specifies number of bytes to be read.
  Buffer | specifies a pointer to u8 variable that will be filled with data.
  Stop | specifies the stop flag which is either TRUE/FALSE.

Returns
  - XST_SUCCESS if an acknowledgement received and timeout.
  - XST_FAILURE if no acknowledgement received.

Note
  None.

References XV_HDMITX_DDC_CMD_RD_TOKEN, XV_HDMITX_DDC_CMD_STP_TOKEN, XV_HDMITX_DDC_CMD_STR_TOKEN, XV_HDMITX_DDC_CMD_WR_TOKEN, XV_HdmiTx_DdcDisable, XV_HdmiTx_DdcEnable, XV_HdmiTx_DdcGetAck(), XV_HdmiTx_DdcIntrDisable, XV_HdmiTx_DdcReadData(), XV_HdmiTx_DdcWaitForDone(), XV_HdmiTx_DdcWriteCommand(), XV_HdmiTx_PioIntrDisable, and XV_HdmiTx_PioIntrEnable.

Referenced by XV_HdmiTx_ClockRatio(), XV_HdmiTx_Scrambler(), and XV_HdmiTx_ShowSCDC().

int XV_HdmiTx_DdcWrite | ( | XV_HdmiTx * | InstancePtr,
|  | u8 | Slave,
|  | u16 | Length,
|  | u8 * | Buffer,
|  | u8 | Stop
| ) |  |

This function writes data from DDC peripheral from given slave address.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.
  Slave | specifies the slave address from where data needs to be read.
  Length | specifies number of bytes to be read.
  Buffer | specifies a pointer to u8 variable that will be filled with data.
  Stop | specifies the stop flag which is either TRUE/FALSE.

Returns
  - XST_SUCCESS if an acknowledgement received and timeout.
  - XST_FAILURE if no acknowledgement received.

Note
  None.

References XV_HDMITX_DDC_CMD_STP_TOKEN, XV_HDMITX_DDC_CMD_STR_TOKEN, XV_HDMITX_DDC_CMD_WR_TOKEN, XV_HdmiTx_DdcDisable, XV_HdmiTx_DdcEnable, XV_HdmiTx_DdcGetAck(), XV_HdmiTx_DdcIntrDisable, XV_HdmiTx_DdcWaitForDone(), XV_HdmiTx_DdcWriteCommand(), XV_HdmiTx_PioIntrDisable, and XV_HdmiTx_PioIntrEnable.

Referenced by XV_HdmiTx_ClockRatio(), XV_HdmiTx_DetectHdmi20(), XV_HdmiTx_Scrambler(), and XV_HdmiTx_ShowSCDC().

void XV_HdmiTx_DebugInfo | ( | XV_HdmiTx * | InstancePtr | ) |

This function prints stream and timing information on STDIO/Uart console.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  None.

References XV_HdmiTx::Stream, and XV_HdmiTx_Stream::Video.

int XV_HdmiTx_DetectHdmi20 | ( | XV_HdmiTx * | InstancePtr | ) |

This function detects connected sink is a HDMI 2.0/HDMI 1.4 sink device and sets appropriate flag in the TX stream.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  - XST_SUCCESS if HDMI 2.0
  - XST_FAILURE if HDMI 1.4

Note
  None.

References XV_HdmiTx_Stream::IsHdmi20, XV_HdmiTx::Stream, and XV_HdmiTx_DdcWrite().

void XV_HdmiTx_EXT_SYSRST | ( | XV_HdmiTx * | InstancePtr,
|  | u8 | Reset
| ) |  |

This function asserts or releases the HDMI TX External SYSRST.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.
  Reset | specifies TRUE/FALSE value to either assert or release HDMI TX External SYSRST.

Returns
  None.

Note
  The reset output of the PIO is inverted. When the system is in reset, the PIO output is cleared and this will reset the HDMI TX. Therefore, clearing the PIO reset output will assert the HDMI External system reset. C-style signature: void XV_HdmiTx_EXT_SYSRST(XV_HdmiTx *InstancePtr, u8 Reset)

References XV_HDMITX_PIO_OUT_CLR_OFFSET, XV_HDMITX_PIO_OUT_EXT_SYSRST_MASK, XV_HDMITX_PIO_OUT_SET_OFFSET, and XV_HdmiTx_WriteReg.

void XV_HdmiTx_EXT_VRST | ( | XV_HdmiTx * | InstancePtr,
|  | u8 | Reset
| ) |  |

This function asserts or releases the HDMI TX External VRST.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.
  Reset | specifies TRUE/FALSE value to either assert or release HDMI TX External VRST.

Returns
  None.

Note
  The reset output of the PIO is inverted. When the system is in reset, the PIO output is cleared and this will reset the HDMI TX. Therefore, clearing the PIO reset output will assert the HDMI external video reset. C-style signature: void XV_HdmiTx_EXT_VRST(XV_HdmiTx *InstancePtr, u8 Reset)

References XV_HDMITX_PIO_OUT_CLR_OFFSET, XV_HDMITX_PIO_OUT_EXT_VRST_MASK, XV_HDMITX_PIO_OUT_SET_OFFSET, and XV_HdmiTx_WriteReg.

XV_HdmiTx_AudioFormatType XV_HdmiTx_GetAudioFormat | ( | XV_HdmiTx * | InstancePtr | ) |

This function gets the active audio format.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  Active audio format of HDMI Tx

Note
  None.

References XV_HDMITX_AUD_CTRL_AUDFMT_MASK, XV_HDMITX_AUD_CTRL_AUDFMT_SHIFT, XV_HDMITX_AUD_CTRL_OFFSET, and XV_HdmiTx_ReadReg.

u32 XV_HdmiTx_GetTmdsClk | ( | XV_HdmiTx * | InstancePtr,
|  | XVidC_VideoMode | VideoMode,
|  | XVidC_ColorFormat | ColorFormat,
|  | XVidC_ColorDepth | Bpc
| ) |  |

This function sets and return the TMDS Clock based on Video Parameter.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.
  VideoMode | specifies resolution identifier.
  ColorFormat | specifies the type of color format. 0 = XVIDC_CSF_RGB 1 = XVIDC_CSF_YCRCB_444 2 = XVIDC_CSF_YCRCB_422 3 = XVIDC_CSF_YCRCB_420
  Bpc | specifies the color depth/bits per color component. 6 = XVIDC_BPC_6 8 = XVIDC_BPC_8 10 = XVIDC_BPC_10 12 = XVIDC_BPC_12 16 = XVIDC_BPC_16

Returns
  - TMDS Clock

Note
  None.

References XV_HdmiTx_Stream::PixelClk, and XV_HdmiTx::Stream.

Referenced by XV_HdmiTx_SetStream().

void XV_HdmiTx_INT_LRST | ( | XV_HdmiTx * | InstancePtr,
|  | u8 | Reset
| ) |  |

This function asserts or releases the HDMI TX Internal LRST.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.
  Reset | specifies TRUE/FALSE value to either assert or release HDMI TX Internal LRST.

Returns
  None.

Note
  The reset output of the PIO is inverted. When the system is in reset, the PIO output is cleared and this will reset the HDMI TX. Therefore, clearing the PIO reset output will assert the HDMI Internal link reset. C-style signature: void XV_HdmiTx_INT_VRST(XV_HdmiTx *InstancePtr, u8 Reset)

References XV_HDMITX_PIO_OUT_CLR_OFFSET, XV_HDMITX_PIO_OUT_INT_LRST_MASK, XV_HDMITX_PIO_OUT_SET_OFFSET, and XV_HdmiTx_WriteReg.

void XV_HdmiTx_INT_VRST | ( | XV_HdmiTx * | InstancePtr,
|  | u8 | Reset
| ) |  |

This function asserts or releases the HDMI TX Internal VRST.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.
  Reset | specifies TRUE/FALSE value to either assert or release HDMI TX Internal VRST.

Returns
  None.

Note
  The reset output of the PIO is inverted. When the system is in reset, the PIO output is cleared and this will reset the HDMI TX. Therefore, clearing the PIO reset output will assert the HDMI Internal video reset. C-style signature: void XV_HdmiTx_INT_VRST(XV_HdmiTx *InstancePtr, u8 Reset)

References XV_HDMITX_PIO_OUT_CLR_OFFSET, XV_HDMITX_PIO_OUT_INT_VRST_MASK, XV_HDMITX_PIO_OUT_SET_OFFSET, and XV_HdmiTx_WriteReg.

void XV_HdmiTx_IntrHandler | ( | void * | InstancePtr | ) |

This function is the interrupt handler for the HDMI TX driver.

This handler reads the pending interrupt from PIO and DDC peripheral, determines the source of the interrupts, clears the interrupts and calls callbacks accordingly.

The application is responsible for connecting this function to the interrupt system. Application beyond this driver is also responsible for providing callbacks to handle interrupts and installing the callbacks using XV_HdmiTx_SetCallback() during initialization phase. An example delivered with this driver demonstrates how this could be done.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx instance that just interrupted.

Returns
  None.

Note
  None.

References XV_HdmiTx_Config::BaseAddress, XV_HdmiTx::Config, XV_HdmiTx::IsReady, XV_HDMITX_DDC_STA_IRQ_MASK, XV_HDMITX_DDC_STA_OFFSET, XV_HDMITX_PIO_STA_IRQ_MASK, XV_HDMITX_PIO_STA_OFFSET, and XV_HdmiTx_ReadReg.

int XV_HdmiTx_IsStreamConnected | ( | XV_HdmiTx * | InstancePtr | ) |

This function provides the stream connected status.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  - TRUE = Stream is connected.
  - FALSE = Stream is connected.

Note
  None.

References XV_HdmiTx_Stream::IsConnected, and XV_HdmiTx::Stream.

int XV_HdmiTx_IsStreamScrambled | ( | XV_HdmiTx * | InstancePtr | ) |

This function provides status of the stream.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  - TRUE = Scrambled.
  - FALSE = Not scrambled.

Note
  None.

References XV_HdmiTx_Stream::IsScrambled, and XV_HdmiTx::Stream.

XV_HdmiTx_Config* XV_HdmiTx_LookupConfig | ( | u16 | DeviceId | ) |

This function returns a reference to an XV_HdmiTx_Config structure based on the core id, DeviceId.

The return value will refer to an entry in the device configuration table defined in the xv_hdmitx_g.c file.

Parameters

  DeviceId | is the unique core ID of the HDMI TX core for the lookup operation.

Returns
  XV_HdmiTx_LookupConfig returns a reference to a config record in the configuration table (in xv_hdmitx_g.c) corresponding to DeviceId, or NULL if no match is found.

Note
  None.

int XV_HdmiTx_Scrambler | ( | XV_HdmiTx * | InstancePtr | ) |

This function controls the scrambler.

Requires TMDSClock to be up to date in order to force enable scrambler when TMDSClock > 340MHz.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  - XST_SUCCESS if HDMI 2.0
  - XST_FAILURE if HDMI 1.4

Note
  None.

References XV_HdmiTx_Stream::IsHdmi20, XV_HdmiTx_Stream::IsScrambled, XV_HdmiTx_Stream::OverrideScrambler, XV_HdmiTx::Stream, XV_HdmiTx_Stream::TMDSClock, XV_HdmiTx_DdcRead(), XV_HdmiTx_DdcWrite(), and XV_HdmiTx_SetScrambler.

Referenced by XV_HdmiTx_SetStream().

int XV_HdmiTx_SelfTest | ( | XV_HdmiTx * | InstancePtr | ) |

This function reads ID of HDMI TX PIO peripheral.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  - XST_SUCCESS if PIO ID was matched.
  - XST_FAILURE if PIO ID was mismatched.

Note
  None.

References XV_HdmiTx_Config::BaseAddress, XV_HdmiTx::Config, XV_HDMITX_MASK_16, XV_HDMITX_PIO_ID, XV_HDMITX_PIO_ID_OFFSET, XV_HdmiTx_ReadReg, and XV_HDMITX_SHIFT_16.

int XV_HdmiTx_SetAudioChannels | ( | XV_HdmiTx * | InstancePtr,
|  | u8 | Value
| ) |  |

This function sets the active audio channels.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  - XST_SUCCESS if active channels were set.
  - XST_FAILURE if no active channles were set.

Note
  None.

References XV_HDMITX_AUD_CTRL_CH_MASK, XV_HDMITX_AUD_CTRL_CH_SHIFT, XV_HDMITX_AUD_CTRL_CLR_OFFSET, XV_HDMITX_AUD_CTRL_OFFSET, XV_HDMITX_AUD_CTRL_RUN_MASK, XV_HDMITX_AUD_CTRL_SET_OFFSET, XV_HdmiTx_ReadReg, and XV_HdmiTx_WriteReg.

int XV_HdmiTx_SetAudioFormat | ( | XV_HdmiTx * | InstancePtr,
|  | XV_HdmiTx_AudioFormatType | Value
| ) |  |

This function sets the active audio format.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  - XST_SUCCESS if active channels were set.
  - XST_FAILURE if no active channles were set.

Note
  None.

References XV_HDMITX_AUD_CTRL_AUDFMT_MASK, XV_HDMITX_AUD_CTRL_AUDFMT_SHIFT, XV_HDMITX_AUD_CTRL_CLR_OFFSET, XV_HDMITX_AUD_CTRL_OFFSET, XV_HDMITX_AUD_CTRL_RUN_MASK, XV_HDMITX_AUD_CTRL_SET_OFFSET, XV_HdmiTx_ReadReg, and XV_HdmiTx_WriteReg.

void XV_HdmiTx_SetAxiClkFreq | ( | XV_HdmiTx * | InstancePtr,
|  | u32 | ClkFreq
| ) |  |

This function sets the AXI4-Lite Clock Frequency.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.
  ClkFreq | specifies the value that needs to be set.

Returns

Note
  This is required after a reset or init.

References XV_HdmiTx_DdcInit().

int XV_HdmiTx_SetCallback | ( | XV_HdmiTx * | InstancePtr,
|  | XV_HdmiTx_HandlerType | HandlerType,
|  | void * | CallbackFunc,
|  | void * | CallbackRef
| ) |  |

This function installs an asynchronous callback function for the given HandlerType:

    HandlerType              Callback Function Type
    -----------------------  --------------------------------------------------
    (XV_HDMITX_HANDLER_HPD)   HpdCallback
    (XV_HDMITX_HANDLER_VS)    VsCallback

Parameters

  InstancePtr | is a pointer to the HDMI TX core instance.
  HandlerType | specifies the type of handler.
  CallbackFunc | is the address of the callback function.
  CallbackRef | is a user data item that will be passed to the callback function when it is invoked.

Returns
  - XST_SUCCESS if callback function installed successfully.
  - XST_INVALID_PARAM when HandlerType is invalid.

Note
  Invoking this function for a handler that already has been installed replaces it with the new handler.

References XV_HdmiTx::BrdgOverflowCallback, XV_HdmiTx::BrdgOverflowRef, XV_HdmiTx::BrdgUnderflowCallback, XV_HdmiTx::BrdgUnderflowRef, XV_HdmiTx::BrdgUnlockedCallback, XV_HdmiTx::BrdgUnlockedRef, XV_HdmiTx::ConnectCallback, XV_HdmiTx::ConnectRef, XV_HdmiTx::IsBrdgOverflowCallbackSet, XV_HdmiTx::IsBrdgUnderflowCallbackSet, XV_HdmiTx::IsBrdgUnlockedCallbackSet, XV_HdmiTx::IsConnectCallbackSet, XV_HdmiTx::IsStreamDownCallbackSet, XV_HdmiTx::IsStreamUpCallbackSet, XV_HdmiTx::IsToggleCallbackSet, XV_HdmiTx::IsVsCallbackSet, XV_HdmiTx::StreamDownCallback, XV_HdmiTx::StreamDownRef, XV_HdmiTx::StreamUpCallback, XV_HdmiTx::StreamUpRef, XV_HdmiTx::ToggleCallback, XV_HdmiTx::ToggleRef, XV_HdmiTx::VsCallback, and XV_HdmiTx::VsRef.

void XV_HdmiTx_SetColorDepth | ( | XV_HdmiTx * | InstancePtr | ) |

This function sets the color depth.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  None.

References XV_HdmiTx_Config::BaseAddress, XV_HdmiTx::Config, XV_HdmiTx::Stream, XV_HdmiTx_Stream::Video, XV_HDMITX_PIO_OUT_COLOR_DEPTH_MASK, XV_HDMITX_PIO_OUT_COLOR_DEPTH_SHIFT, XV_HDMITX_PIO_OUT_MSK_OFFSET, XV_HDMITX_PIO_OUT_OFFSET, and XV_HdmiTx_WriteReg.

Referenced by XV_HdmiTx_SetStream().

void XV_HdmiTx_SetColorFormat | ( | XV_HdmiTx * | InstancePtr | ) |

This function sets the color format.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  None.

References XV_HdmiTx_Config::BaseAddress, XV_HdmiTx::Config, XV_HdmiTx::Stream, XV_HdmiTx_Stream::Video, XV_HDMITX_PIO_OUT_COLOR_SPACE_MASK, XV_HDMITX_PIO_OUT_COLOR_SPACE_SHIFT, XV_HDMITX_PIO_OUT_MSK_OFFSET, XV_HDMITX_PIO_OUT_OFFSET, and XV_HdmiTx_WriteReg.

Referenced by XV_HdmiTx_SetStream().

void XV_HdmiTx_SetDviMode | ( | XV_HdmiTx * | InstancePtr | ) |

This function sets the core into DVI mode.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns

Note
  This is required after a reset or init.

References XV_HdmiTx_Stream::IsHdmi, XV_HdmiTx::Stream, XV_HdmiTx_AudioDisable, XV_HdmiTx_AuxDisable, and XV_HdmiTx_ClearMode.

void XV_HdmiTx_SetGcpAvmuteBit | ( | XV_HdmiTx * | InstancePtr | ) |

This function sets the HDMI TX AUX GCP register AVMUTE bit.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  None.

References XV_HDMITX_PIO_OUT_GCP_AVMUTE_MASK, XV_HDMITX_PIO_OUT_SET_OFFSET, and XV_HdmiTx_WriteReg.

void XV_HdmiTx_SetGcpClearAvmuteBit | ( | XV_HdmiTx * | InstancePtr | ) |

This function sets the HDMI TX AUX GCP register CLEAR_AVMUTE bit.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  None.

References XV_HDMITX_PIO_OUT_GCP_CLEARAVMUTE_MASK, XV_HDMITX_PIO_OUT_SET_OFFSET, and XV_HdmiTx_WriteReg.

void XV_HdmiTx_SetHdmiMode | ( | XV_HdmiTx * | InstancePtr | ) |

This function sets the core into HDMI mode.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns

Note
  This is required after a reset or init.

References XV_HdmiTx_Stream::IsHdmi, XV_HdmiTx::Stream, XV_HdmiTx_AudioEnable, XV_HdmiTx_AuxEnable, and XV_HdmiTx_SetMode.

Referenced by XV_HdmiTx_CfgInitialize().

void XV_HdmiTx_SetPixelRate | ( | XV_HdmiTx * | InstancePtr | ) |

This function sets the pixel rate at output.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  None.

References XV_HdmiTx_Config::BaseAddress, XV_HdmiTx::Config, XV_HdmiTx::Stream, XV_HdmiTx_Stream::Video, XV_HDMITX_PIO_OUT_MSK_OFFSET, XV_HDMITX_PIO_OUT_OFFSET, XV_HDMITX_PIO_OUT_PIXEL_RATE_MASK, XV_HDMITX_PIO_OUT_PIXEL_RATE_SHIFT, and XV_HdmiTx_WriteReg.

Referenced by XV_HdmiTx_SetStream().

void XV_HdmiTx_SetSampleRate | ( | XV_HdmiTx * | InstancePtr,
|  | u8 | SampleRate
| ) |  |

This function sets the sample rate at output.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.
  SampleRate | specifies the value that needs to be set. 2 samples per clock 3 samples per clock. 5 samples per clock.

Returns
  None.

Note
  None.

References XV_HdmiTx_Config::BaseAddress, XV_HdmiTx::Config, XV_HdmiTx_Stream::SampleRate, XV_HdmiTx::Stream, XV_HDMITX_PIO_OUT_MSK_OFFSET, XV_HDMITX_PIO_OUT_OFFSET, XV_HDMITX_PIO_OUT_SAMPLE_RATE_MASK, XV_HDMITX_PIO_OUT_SAMPLE_RATE_SHIFT, and XV_HdmiTx_WriteReg.

u32 XV_HdmiTx_SetStream | ( | XV_HdmiTx * | InstancePtr,
|  | XVidC_VideoMode | VideoMode,
|  | XVidC_ColorFormat | ColorFormat,
|  | XVidC_ColorDepth | Bpc,
|  | XVidC_PixelsPerClock | Ppc,
|  | XVidC_3DInfo * | Info3D
| ) |  |

This function sets the HDMI TX stream parameters.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.
  VideoMode | specifies resolution identifier.
  ColorFormat | specifies the type of color format. 0 = XVIDC_CSF_RGB 1 = XVIDC_CSF_YCRCB_444 2 = XVIDC_CSF_YCRCB_422 3 = XVIDC_CSF_YCRCB_420
  Bpc | specifies the color depth/bits per color component. 6 = XVIDC_BPC_6 8 = XVIDC_BPC_8 10 = XVIDC_BPC_10 12 = XVIDC_BPC_12 16 = XVIDC_BPC_16
  Ppc | specifies the pixel per clock. 1 = XVIDC_PPC_1 2 = XVIDC_PPC_2 4 = XVIDC_PPC_4

Returns
  TmdsClock, reference clock calculated based on the input parameters.

Note
  None.

In HDMI the colordepth in YUV422 is always 12 bits, although on the link itself it is being transmitted as 8-bits. Therefore if the colorspace is YUV422, then force the colordepth to 12 bits.

References XV_HdmiTx_Stream::IsHdmi20, XV_HdmiTx_Stream::IsScrambled, XV_HdmiTx::Stream, XV_HdmiTx_Stream::TMDSClock, XV_HdmiTx_Stream::TMDSClockRatio, XV_HdmiTx_Stream::Vic, XV_HdmiTx_Stream::Video, XV_HdmiTx_ClockRatio(), XV_HdmiTx_GetTmdsClk(), XV_HdmiTx_LookupVic(), XV_HdmiTx_Scrambler(), XV_HdmiTx_SetColorDepth(), XV_HdmiTx_SetColorFormat(), and XV_HdmiTx_SetPixelRate().

void XV_HdmiTx_ShowSCDC | ( | XV_HdmiTx * | InstancePtr | ) |

This function shows the sinks SCDC registers.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx core instance.

Returns
  None.

Note
  None.

References XV_HdmiTx_DdcRead(), and XV_HdmiTx_DdcWrite().

char* XV_HdmiTx_VSIF_3DSampMethodToString | ( | XV_HdmiTx_3D_Sampling_Method | Item | ) |

This function returns a string representation of the enumerated type XV_HdmiTx_3D_Sampling_Method.

Parameters

  Item | specifies the value to convert.

Returns
  Pointer to the converted string.

References XV_HDMITX_3D_SAMPLING_HORIZONTAL, and XV_HDMITX_3D_SAMPLING_QUINCUNX.

Referenced by XV_HdmiTx_VSIF_DisplayInfo().

char* XV_HdmiTx_VSIF_3DSampPosToString | ( | XV_HdmiTx_3D_Sampling_Position | Item | ) |

This function returns a string representation of the enumerated type XV_HdmiTx_3D_Sampling_Position.

Parameters

  Item | specifies the value to convert.

Returns
  Pointer to the converted string.

References XV_HDMITX_3D_SAMPPOS_ELER, XV_HDMITX_3D_SAMPPOS_ELOR, XV_HDMITX_3D_SAMPPOS_OLER, and XV_HDMITX_3D_SAMPPOS_OLOR.

Referenced by XV_HdmiTx_VSIF_DisplayInfo().

char* XV_HdmiTx_VSIF_3DStructToString | ( | XV_HdmiTx_3D_Struct_Field | Item | ) |

This function returns a string representation of the enumerated type XV_HdmiTx_3D_Struct_Field.

Parameters

  Item | specifies the value to convert.

Returns
  Pointer to the converted string.

References XV_HDMITX_3D_STRUCT_FIELD_ALTERNATIVE, XV_HDMITX_3D_STRUCT_FRAME_PACKING, XV_HDMITX_3D_STRUCT_L_DEPTH, XV_HDMITX_3D_STRUCT_L_DEPTH_GRAPH_GDEPTH, XV_HDMITX_3D_STRUCT_LINE_ALTERNATIVE, XV_HDMITX_3D_STRUCT_SIDE_BY_SIDE_FULL, XV_HDMITX_3D_STRUCT_SIDE_BY_SIDE_HALF, and XV_HDMITX_3D_STRUCT_TOP_AND_BOTTOM.

Referenced by XV_HdmiTx_VSIF_DisplayInfo().

void XV_HdmiTx_VSIF_DisplayInfo | ( | XV_HdmiTx_VSIF * | VSIFPtr | ) |

This function displays the contents of an XV_HdmiTx_VSIF instance.

Parameters

  VSIFPtr | is a pointer to the XV_HdmiTx_VSIF instance.

Returns
  None.

References XV_HdmiTx_VSIF::Format, XV_HdmiTx_VSIF::HDMI_VIC, XV_HdmiTx_VSIF::Info_3D, XV_HdmiTx_3D_MetaData::IsPresent, XV_HdmiTx_3D_Info::MetaData, XV_HDMITX_3D_STRUCT_SIDE_BY_SIDE_HALF, XV_HdmiTx_VSIF_3DSampMethodToString(), XV_HdmiTx_VSIF_3DSampPosToString(), XV_HdmiTx_VSIF_3DStructToString(), XV_HDMITX_VSIF_VF_3D, and XV_HDMITX_VSIF_VF_EXTRES.

int XV_HdmiTx_VSIF_GeneratePacket | ( | XV_HdmiTx_VSIF * | VSIFPtr,
|  | XHdmiC_Aux * | AuxPtr
| ) |  |

This function generates a Vendor Specific InfoFrame (VSIF).

Parameters

  VSIFPtr | is a pointer to the XV_HdmiTx_VSIF instance.
  AuxPtr | is a pointer to the XV_HdmiTx_Tx_Aux instance.

Returns
  - XST_SUCCESS if operation was successful
  - XST_FAILURE if an error was detected during generation

References XV_HdmiTx_3D_MetaData::Data, XV_HdmiTx_VSIF::Format, XV_HdmiTx_VSIF::HDMI_VIC, XV_HdmiTx_VSIF::IEEE_ID, XV_HdmiTx_VSIF::Info_3D, XV_HdmiTx_3D_MetaData::IsPresent, XV_HdmiTx_3D_MetaData::Length, XV_HdmiTx_3D_Info::MetaData, XV_HdmiTx_3D_MetaData::Type, XV_HdmiTx_VSIF::Version, XV_HDMITX_3D_STRUCT_SIDE_BY_SIDE_HALF, XV_HDMITX_VSIF_VF_3D, and XV_HDMITX_VSIF_VF_EXTRES.