| v_hdmitx1 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

Functions
xv_hdmitx1_selftest.c File Reference

## Overview

This file contains self test function for the HDMI TX core.

    MODIFICATION HISTORY:

    Ver   Who    Date     Changes

    1.00  EB     22/05/18 Initial release.

## Functions
int | XV_HdmiTx1_SelfTest (XV_HdmiTx1 *InstancePtr)
| This function reads ID of HDMI TX PIO peripheral. More...

## Function Documentation

int XV_HdmiTx1_SelfTest | ( | XV_HdmiTx1 * | InstancePtr | ) |

This function reads ID of HDMI TX PIO peripheral.

Parameters

  InstancePtr | is a pointer to the XV_HdmiTx1 core instance.

Returns
  - XST_SUCCESS if PIO ID was matched.
  - XST_FAILURE if PIO ID was mismatched.

Note
  None.

References XV_HdmiTx1_Config::BaseAddress, XV_HdmiTx1::Config, XV_HDMITX1_MASK_16, XV_HDMITX1_PIO_ID, XV_HDMITX1_PIO_ID_OFFSET, XV_HdmiTx1_ReadReg, and XV_HDMITX1_SHIFT_16.