| aiengine Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XAieGbl_Config Struct Reference

This typedef contains configuration information for the device. More...

## Data Fields
u16 | DeviceId
| Unique ID of the AIE device. More...
u32 | ArrOffset
| AIE array address offset in the system address map. More...
u16 | NumRows
| Total number of rows including shim. More...
u16 | NumCols
| Total number of columns. More...

## Detailed Description

This typedef contains configuration information for the device.

## Field Documentation

u32 XAieGbl_Config::ArrOffset

AIE array address offset in the system address map.

Referenced by XAieGbl_CfgInitialize(), and XAieGbl_HwInit().

u16 XAieGbl_Config::DeviceId

Unique ID of the AIE device.

u16 XAieGbl_Config::NumCols

Total number of columns.

Referenced by XAieGbl_CfgInitialize(), XAieGbl_HwInit(), and XAieSim_GetTargetTileAddr().

u16 XAieGbl_Config::NumRows

Total number of rows including shim.

Referenced by XAieGbl_CfgInitialize(), XAieGbl_HwInit(), XAieSim_GetTargetTileAddr(), and XAieTile_CoreEventStatusClear().