| dmaps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

- All
- Variables

- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- p
- s
- u

Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - a -

- Allocated : XDmaPs_ProgBuf

### - b -

- BaseAddress : XDmaPs_Config
- BD : XDmaPs_Cmd
- Buf : XDmaPs_ProgBuf

### - c -

- CacheLength : XDmaPs
- ChanCtrl : XDmaPs_Cmd
- ChanFaultPCAddr : XDmaPs_Cmd
- ChanFaultType : XDmaPs_Cmd
- ChanId : XDmaPs_ChannelData
- Chans : XDmaPs
- Config : XDmaPs

### - d -

- DeviceId : XDmaPs_Config
- DevId : XDmaPs_ChannelData
- DmaCmdFromHw : XDmaPs_ChannelData
- DmaCmdToHw : XDmaPs_ChannelData
- DmaStatus : XDmaPs_Cmd
- DoneHandler : XDmaPs_ChannelData
- DoneRef : XDmaPs_ChannelData
- DstAddr : XDmaPs_BD
- DstBurstLen : XDmaPs_ChanCtrl
- DstBurstSize : XDmaPs_ChanCtrl
- DstCacheCtrl : XDmaPs_ChanCtrl
- DstInc : XDmaPs_ChanCtrl
- DstProtCtrl : XDmaPs_ChanCtrl

### - e -

- EndianSwapSize : XDmaPs_ChanCtrl

### - f -

- FaultHandler : XDmaPs
- FaultRef : XDmaPs

### - g -

- GeneratedDmaProg : XDmaPs_Cmd
- GeneratedDmaProgLength : XDmaPs_Cmd

### - h -

- HoldDmaProg : XDmaPs_ChannelData

### - i -

- IsReady : XDmaPs

### - l -

- Len : XDmaPs_ProgBuf
- Length : XDmaPs_BD

### - p -

- ProgBufPool : XDmaPs_ChannelData

### - s -

- SrcAddr : XDmaPs_BD
- SrcBurstLen : XDmaPs_ChanCtrl
- SrcBurstSize : XDmaPs_ChanCtrl
- SrcCacheCtrl : XDmaPs_ChanCtrl
- SrcInc : XDmaPs_ChanCtrl
- SrcProtCtrl : XDmaPs_ChanCtrl

### - u -

- UserDmaProg : XDmaPs_Cmd
- UserDmaProgLength : XDmaPs_Cmd