| qspipsu Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Macros
xqspipsu_flash_config.h File Reference

## Overview

This file contains flash configuration table and flash related defines.

This file should be included in the example files and compiled along with the examples (*.c).

Note

None.

     MODIFICATION HISTORY:

     Ver   Who Date     Changes

     1.12  akm 07/07/20 First release
     1.12   akm 07/07/20 Add support for Macronix flash(MX66U2G45G, MX66L2G45G)
                        and ISSI flash(IS25LP01G, IS25WP01G) parts.
     1.13  akm 12/10/20 Set Read command as per the qspi bus width.
     1.14  akm 07/16/21 Enable Quad Mode for Winbond flashes.
     1.15  akm 11/19/21 Fix read/write failures on Spansion flash parts.
     1.17  akm 10/31/22 Add support for Winbond flash w25q02nw.
     1.18  sb  05/19/23 Update number of sector calculation logic
               in flash erase API.
     1.19  sb  11/10/23 Add support for Winbond flash w25q256jw
     1.19  sb  11/10/23 Add support for ISSI flash is25lp02g
     1.20  sb  05/20/24 Add support for ISSI flash is25lp01gg
     1.20  sb  09/13/24 Updated examples to configure correct baud rate value

## Macros
#define | ISSI_ID_BYTE0 0x9D
| Maximum delay count. More...

## Macro Definition Documentation

#define ISSI_ID_BYTE0 0x9D

Maximum delay count.

Referenced by FlashEnableQuadMode(), and FlashEnterExit4BAddMode().