| uartns550 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XUartNs550_Config Struct Reference
Overview

This typedef contains configuration information for the device. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
UINTPTR | BaseAddress
| Base address of device. More...
u32 | InputClockHz
| Input clock frequency. More...
u32 | DefaultBaudRate
| Baud Rate in bps, ie 1200. More...

## Detailed Description

This typedef contains configuration information for the device.

## Field Documentation

UINTPTR XUartNs550_Config::BaseAddress

Base address of device.

Referenced by XUartNs550_Initialize().

u32 XUartNs550_Config::DefaultBaudRate

Baud Rate in bps, ie 1200.

Referenced by XUartNs550_CfgInitialize(), and XUartNs550_Initialize().

u16 XUartNs550_Config::DeviceId

Unique ID of device.

u32 XUartNs550_Config::InputClockHz

Input clock frequency.

Referenced by XUartNs550_CfgInitialize().