| mipi_tx_phy Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XMipi_Tx_Phy Struct Reference
Overview

The Xmipi_tx_phy Controller driver instance data. More...

## Data Fields
XMipi_Tx_Phy_Config | Config
| Hardware Configuration. More...
u32 | IsReady
| Driver is ready. More...

## Detailed Description

The Xmipi_tx_phy Controller driver instance data.

The user is required to allocate a variable of this type for every Xmipi_tx_phy device in the system. A pointer to a variable of this type is then passed to the driver API functions.

## Field Documentation

XMipi_Tx_Phy_Config XMipi_Tx_Phy::Config

Hardware Configuration.

Referenced by XMipi_Tx_Phy_Activate(), XMipi_Tx_Phy_CfgInitialize(), XMipi_Tx_Phy_ClearDataLane(), XMipi_Tx_Phy_Configure(), XMipi_Tx_Phy_GetClkLaneMode(), XMipi_Tx_Phy_GetClkLaneStatus(), XMipi_Tx_Phy_GetDataLaneMode(), XMipi_Tx_Phy_GetDataLaneStatus(), XMipi_Tx_Phy_GetDLCalibStatus(), XMipi_Tx_Phy_GetInfo(), XMipi_Tx_Phy_GetPacketCount(), XMipi_Tx_Phy_GetRegIntfcPresent(), XMipi_Tx_Phy_GetVersionReg(), XMipi_Tx_Phy_Reset(), and XMipi_Tx_Phy_SelfTest().

u32 XMipi_Tx_Phy::IsReady

Driver is ready.

Referenced by XMipi_Tx_Phy_CfgInitialize(), and XMipi_Tx_Phy_Reset().