| dp14txss Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

Functions
dppt_vid_phy_config.h File Reference

## Overview

This file contains functions to configure Video Pattern Generator core.

    MODIFICATION HISTORY:

    Ver   Who    Date     Changes

    1.00  KI    07/13/17 Initial release.

## Functions
void | PLLRefClkSel (XVphy *InstancePtr, u8 link_rate)
| This function sets proper ref clk frequency and line rate. More...
u32 | PHY_Configuration_Tx (XVphy *InstancePtr, XVphy_User_Config PHY_User_Config_Table)
| This function sets up PHY. More...

## Function Documentation

u32 PHY_Configuration_Tx | ( | XVphy * | InstancePtr,
|  | XVphy_User_Config | PHY_User_Config_Table
| ) |  |

This function sets up PHY.

Parameters

  pointer | to VideoPHY
  User | Config table

Returns
  - XST_SUCCESS if interrupt setup was successful.
  - A specific error code defined in "xstatus.h" if an error occurs.

Note
  None.

void PLLRefClkSel | ( | XVphy * | InstancePtr,
|  | u8 | link_rate
| ) |  |

This function sets proper ref clk frequency and line rate.

Parameters

  InstancePtr | is a pointer to the Video PHY instance.

Returns
  None.

Note
  None.