| dp21 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XDp_TxBoardChar Struct Reference
Overview

This typedef describes some board characteristics information that affects link training. More...

## Data Fields
u8 | HasRedriverInPath
| Redriver in path requires different voltage swing and pre-emphasis. More...
u8 | TxVsLevels [4]
| The voltage swing levels to be used by the DisplayPort TX. More...
u8 | TxPeLevels [4]
| The pre-emphasis/cursor level to be used by the DisplayPort TX. More...
u8 | TxVsOffset
| Voltage swing compensation offset used when pre-emphasis is used. More...

## Detailed Description

This typedef describes some board characteristics information that affects link training.

## Field Documentation

u8 XDp_TxBoardChar::HasRedriverInPath

Redriver in path requires different voltage swing and pre-emphasis.

u8 XDp_TxBoardChar::TxPeLevels[4]

The pre-emphasis/cursor level to be used by the DisplayPort TX.

u8 XDp_TxBoardChar::TxVsLevels[4]

The voltage swing levels to be used by the DisplayPort TX.

u8 XDp_TxBoardChar::TxVsOffset

Voltage swing compensation offset used when pre-emphasis is used.