| qspipsu Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Macros | Functions
xqspipsu_xfer.c File Reference

## Macros
#define | MAX_DELAY_CNT 1000000000U
| Max delay count. More...

## Functions
s32 | XQspiPsu_PolledSendData (XQspiPsu *InstancePtr, XQspiPsu_Msg *Msg, s32 Index)
| Transfers Tx data on the bus in polled mode. More...
s32 | XQspiPsu_PolledRecvData (XQspiPsu *InstancePtr, XQspiPsu_Msg *Msg, s32 Index, u32 *IOPending)
| Transfers Rx data on the bus in polled mode. More...
void | XQspiPsu_IntrSendData (XQspiPsu *InstancePtr, u32 QspiPsuStatusReg, u8 *DeltaMsgCnt)
| Performs a transfer of Tx data on the bus in interrupt mode. More...
void | XQspiPsu_IntrRecvData (XQspiPsu *InstancePtr, u32 QspiPsuStatusReg, u32 DmaIntrStatusReg, u8 *DeltaMsgCnt)
| Performs a transfer of Rx data on the busin interrupt mode. More...