| ttcps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XTtcPs_Config Struct Reference
Overview

This typedef contains configuration information for the device. More...

## Data Fields
u16 | DeviceId
| Unique ID for device. More...
u32 | BaseAddress
| Base address for device. More...
u32 | InputClockHz
| Input clock frequency. More...

## Detailed Description

This typedef contains configuration information for the device.

## Field Documentation

u32 XTtcPs_Config::BaseAddress

Base address for device.

Referenced by XTtcPs_CfgInitialize(), XTtcPs_GetMatchValue(), XTtcPs_GetOptions(), XTtcPs_GetPrescaler(), XTtcPs_InterruptHandler(), XTtcPs_SelfTest(), XTtcPs_SetMatchValue(), XTtcPs_SetOptions(), XTtcPs_SetPrescaler(), and XTtcPs_SetStatusHandler().

u16 XTtcPs_Config::DeviceId

Unique ID for device.

Referenced by XTtcPs_CfgInitialize(), and XTtcPs_Release().

u32 XTtcPs_Config::InputClockHz

Input clock frequency.

Referenced by XTtcPs_CalcIntervalFromFreq(), and XTtcPs_CfgInitialize().