| uartns550 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Structures
Here are the data structures with brief descriptions:

XUartNs550 | The XUartNs550 driver instance data
XUartNs550_Config | This typedef contains configuration information for the device
XUartNs550Buffer | The following data type is used to manage the buffers that are handled when sending and receiving data in the interrupt mode
XUartNs550Format | This data type allows the data format of the device to be set and retrieved
XUartNs550Stats | UART statistics