.. _ug_wifi_softap_mode:

SoftAP mode
###########

The following subpages describe how an nRF70 Series device operates in :term:`Software-enabled Access Point (SoftAP or SAP)` mode, along with  the memory requirements of Wi-Fi® applications that use the SoftAP mode.

.. toctree::
   :maxdepth: 1
   :caption: Subpages:

   mem_requirements_sap
   sap
