.. _gattp_readme:

Generic Attribute (GATT) Profile
################################

.. contents::
   :local:
   :depth: 2

You can use the GATT Profile library to receive service changed indications from a connected peer.
It is used in the :ref:`peripheral_ancs_client` sample.

API documentation
*****************

| Header file: :file:`include/bluetooth/services/gattp.h`
| Source file: :file:`subsys/bluetooth/services/gattp.c`

.. doxygengroup:: bt_gattp
   :project: nrf
   :members:
