.. _app_event_manager_sample:

Application Event Manager
#########################

.. contents::
   :local:
   :depth: 2

The Application Event Manager sample demonstrates the functionality of the :ref:`app_event_manager` subsystem.
It uses an event-driven architecture, where different modules communicate through sending and processing events.


Overview
********

The sample application consists of three modules that communicate using events:

.. event_manager_sample_modules_start

Sensor (``sensor_simulated.c``):
  This module waits for a configuration event (which is sent by ``main.c``).
  After receiving this event, it simulates measured data at constant intervals.
  Every time the data is updated, the module sends the current values as measurement event.
  When the module receives a control event from the Controller, it responds with an ACK event.

Controller (``controller.c``):
  This module waits for measurement events from the sensor.
  Every time a measurement event is received, the module checks one of the measurement values that are transmitted as part of the event and, if the value exceeds a static threshold, sends a control event.

Statistics (``stats.c``):
  This module waits for measurement events from the sensor.
  The module calculates and logs basic statistics about one of the measurement values that are transmitted as part of the event.

.. event_manager_sample_modules_end

Requirements
************

The sample supports the following development kits:

.. table-from-sample-yaml::

.. include:: /includes/tfm.txt

Configuration
*************

|config|

Building and running
********************
.. |sample path| replace:: :file:`samples/app_event_manager`

.. include:: /includes/build_and_run_ns.txt


Testing
=======

After programming the sample to your development kit, test it by performing the following steps:

1. |connect_terminal|
#. Reset the kit.
#. Observe that output similar to the following is logged on UART::

      ***** Booting Zephyr OS v1.13.99-ncs1-4741-g1d6219f *****
      [00:00:00.000,854] <inf> app_event_manager: e: config_event init_val_1=3
      [00:00:00.001,068] <inf> app_event_manager: e: measurement_event val1=3 val2=3 val3=3
      [00:00:00.509,063] <inf> app_event_manager: e: measurement_event val1=3 val2=6 val3=9
      [00:00:01.018,005] <inf> app_event_manager: e: measurement_event val1=3 val2=9 val3=18
      [00:00:01.526,947] <inf> app_event_manager: e: measurement_event val1=3 val2=12 val3=30
      [00:00:02.035,888] <inf> app_event_manager: e: measurement_event val1=3 val2=15 val3=45
      [00:00:02.035,949] <inf> app_event_manager: e: control_event
      [00:00:02.035,980] <inf> app_event_manager: e: ack_event
      [00:00:02.544,830] <inf> app_event_manager: e: measurement_event val1=-3 val2=12 val3=57
      [00:00:03.053,771] <inf> app_event_manager: e: measurement_event val1=-3 val2=9 val3=66
      [00:00:03.562,713] <inf> app_event_manager: e: measurement_event val1=-3 val2=6 val3=72
      [00:00:04.071,655] <inf> app_event_manager: e: measurement_event val1=-3 val2=3 val3=75
      [00:00:04.580,596] <inf> app_event_manager: e: measurement_event val1=-3 val2=0 val3=75
      [00:00:04.580,596] <inf> stats: Average value3: 45


Dependencies
************

This sample uses the following |NCS| subsystems:

* :ref:`app_event_manager`

In addition, it uses the following Zephyr subsystems:

* :ref:`zephyr:logging_api`

The sample also uses the following secure firmware component:

* :ref:`Trusted Firmware-M <ug_tfm>`
